FILE_TYPE = MULTI_PHYS_TABLE;

PART 'AD623ARMZ'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Analog Devices", "AD623ARMZ" (!) = "", "SOP65P490X110-8N", "Small Outline Packages", "584-AD623ARMZ", "https://www.mouser.co.uk/ProductDetail/Analog-Devices/AD623ARMZ?qs=NmRFExCfTkHh9YiJNpc9iA%3D%3D", "AD623ARMZ, Instrumention Amplifier, 0.5mV Offset, 70dB CMRR, Rail-Rail Output, 3, 5, 9V, 8-Pin MSOP", "http://www.analog.com/static/imported-files/data_sheets/AD623.pdf", "1.1 mm"
END_PART

END.
