<?xml version="1.0" encoding="utf-8"?>
<!--/4689646/1031803/2.50/8/3/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Operational Amplifiers - Op Amps 2-Channel, 1MHz, RRIO, 1.8V to 5.5V Operational Amplifier for Cost-Optimized Systems 8-SOT-23-THIN -40 to 125&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT65P280X110-8N">
<description>&lt;b&gt;DDF0008A&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="TLV9002IDDFR">
<pin name="OUT1" direction="io"/>
<pin name="IN1-" direction="io"/>
<pin name="IN1+" direction="io"/>
<pin name="V-" direction="io"/>
<pin name="IN2+" direction="io"/>
<pin name="IN2-" direction="io"/>
<pin name="OUT2" direction="io"/>
<pin name="V+" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TLV9002IDDFR" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers - Op Amps 2-Channel, 1MHz, RRIO, 1.8V to 5.5V Operational Amplifier for Cost-Optimized Systems 8-SOT-23-THIN -40 to 125&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.ti.com/lit/gpn/TLV9002"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TLV9002IDDFR"/>
</gates>
<devices>
<device name="" package="SOT65P280X110-8N">
<connects>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="IN1-" pad="2"/>
<connect gate="G$1" pin="IN1+" pad="3"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="IN2+" pad="5"/>
<connect gate="G$1" pin="IN2-" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="595-TLV9002IDDFR"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TLV9002IDDFR?qs=mAH9sUMRCtuVJ6NmNV%252Bgrw%3D%3D"/>
<attribute name="Manufacturer_Name" value="Texas Instruments"/>
<attribute name="Manufacturer_Part_Number" value="TLV9002IDDFR"/>
<attribute name="Description" value="Operational Amplifiers - Op Amps 2-Channel, 1MHz, RRIO, 1.8V to 5.5V Operational Amplifier for Cost-Optimized Systems 8-SOT-23-THIN -40 to 125"/>
<attribute name="Height" value="1.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
