(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "TCA9548ARGERQ1" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 26.67 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "TCA9548ARGERQ1" (at 26.67 15.24 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "QFN50P400X400X100-25N-D" (at 26.67 -84.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/gpn/TCA9548A-Q1" (at 26.67 -184.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Automotive 8-channel I2C switch with reset" (at 26.67 -284.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1" (at 26.67 -384.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "595-TCA9548ARGERQ1" (at 26.67 -484.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TCA9548ARGERQ1?qs=T3oQrply3y8QRq0kg9Jjrw%3D%3D" (at 26.67 -584.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Texas Instruments" (at 26.67 -684.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "TCA9548ARGERQ1" (at 26.67 -784.76 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 12.7)
      (end 25.4 -22.86)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "SD0" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "SC0" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "SD1" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "SC1" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "SD2" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "SC2" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 7.62 -27.94 90) (length 5.08)
      (name "SD3" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 -27.94 90) (length 5.08)
      (name "SC3" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 -27.94 90) (length 5.08)
      (name "GND" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 -27.94 90) (length 5.08)
      (name "SD4" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 -27.94 90) (length 5.08)
      (name "SC4" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 -27.94 90) (length 5.08)
      (name "SD5" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 0 180) (length 5.08)
      (name "A2" (effects (font (size 1.27 1.27))))
      (number "18" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -2.54 180) (length 5.08)
      (name "SC7" (effects (font (size 1.27 1.27))))
      (number "17" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -5.08 180) (length 5.08)
      (name "SD7" (effects (font (size 1.27 1.27))))
      (number "16" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -7.62 180) (length 5.08)
      (name "SC6" (effects (font (size 1.27 1.27))))
      (number "15" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -10.16 180) (length 5.08)
      (name "SD6" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -12.7 180) (length 5.08)
      (name "SC5" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 7.62 17.78 270) (length 5.08)
      (name "EP" (effects (font (size 1.27 1.27))))
      (number "25" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 17.78 270) (length 5.08)
      (name "~{RESET}" (effects (font (size 1.27 1.27))))
      (number "24" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 17.78 270) (length 5.08)
      (name "A1" (effects (font (size 1.27 1.27))))
      (number "23" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 17.78 270) (length 5.08)
      (name "A0" (effects (font (size 1.27 1.27))))
      (number "22" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 17.78 270) (length 5.08)
      (name "VCC" (effects (font (size 1.27 1.27))))
      (number "21" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 17.78 270) (length 5.08)
      (name "SDA" (effects (font (size 1.27 1.27))))
      (number "20" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 17.78 270) (length 5.08)
      (name "SCL" (effects (font (size 1.27 1.27))))
      (number "19" (effects (font (size 1.27 1.27))))
    )
  )
)
