(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "VL53L0CXV0DH_1" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 31.75 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "VL53L0CXV0DH_1" (at 31.75 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "LGA12_1" (at 31.75 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/group3/b2/1e/33/77/c6/92/47/6b/DM00279086/files/DM00279086.pdf/jcr:content/translations/en.DM00279086.pdf" (at 31.75 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "STMICROELECTRONICS - VL53L0CXV0DH/1 - GESTURE DETECTION SENSOR, DIGITAL, LGA12" (at 31.75 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "" (at 31.75 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "511-VL53L0CXV0DH/1" (at 31.75 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/VL53L0CXV0DH-1?qs=dTJS0cRn7ojtsK3C9%252BTaSw%3D%3D" (at 31.75 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "STMicroelectronics" (at 31.75 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "VL53L0CXV0DH/1" (at 31.75 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 30.48 -15.24)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin power_in line (at 0 0 0) (length 5.08)
      (name "AVDDVCSEL" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin input line (at 0 -2.54 0) (length 5.08)
      (name "AVSSVCSEL" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin bidirectional line (at 0 -5.08 0) (length 5.08)
      (name "GND" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin input line (at 0 -7.62 0) (length 5.08)
      (name "GND2" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin output line (at 0 -10.16 0) (length 5.08)
      (name "XSHUT" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin power_in line (at 0 -12.7 0) (length 5.08)
      (name "GND3" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin input line (at 35.56 0 180) (length 5.08)
      (name "GPIO1" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin power_in line (at 35.56 -2.54 180) (length 5.08)
      (name "DNC" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin power_in line (at 35.56 -5.08 180) (length 5.08)
      (name "SDA" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin power_in line (at 35.56 -7.62 180) (length 5.08)
      (name "SCL" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin power_in line (at 35.56 -10.16 180) (length 5.08)
      (name "AVDD" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin power_in line (at 35.56 -12.7 180) (length 5.08)
      (name "GND4" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
  )
)
