(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "OA4ZHA33Q" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 20.32 12.7 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "OA4ZHA33Q" (id 1) (at 20.32 10.16 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "QFN16_3P1X3P1X0P5_STM" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "OA4ZHA33Q" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "OA4ZHA33Q" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN16_3P1X3P1X0P5_STM QFN16_3P1X3P1X0P5_STM-M QFN16_3P1X3P1X0P5_STM-L" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OA4ZHA33Q_0_1"
      (polyline
        (pts
          (xy 7.62 7.62)
          (xy 7.62 -40.64)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 -40.64)
          (xy 33.02 -40.64)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 33.02 -40.64)
          (xy 33.02 7.62)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 33.02 7.62)
          (xy 7.62 7.62)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin input line (at 0 -2.54 0) (length 7.62)
        (name "IN1+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -35.56 0) (length 7.62)
        (name "VCC+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 40.64 -15.24 180) (length 7.62)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 0) (length 7.62)
        (name "IN2+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 7.62)
        (name "IN2-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 0 180) (length 7.62)
        (name "OUT2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 -2.54 180) (length 7.62)
        (name "OUT3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -10.16 0) (length 7.62)
        (name "IN3-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -12.7 0) (length 7.62)
        (name "IN3+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 40.64 -17.78 180) (length 7.62)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -33.02 0) (length 7.62)
        (name "VCC-" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -17.78 0) (length 7.62)
        (name "IN4+" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -15.24 0) (length 7.62)
        (name "IN4-" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 -5.08 180) (length 7.62)
        (name "OUT4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 40.64 2.54 180) (length 7.62)
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 0 0) (length 7.62)
        (name "IN1-" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 0 -22.86 0) (length 7.62)
        (name "EPAD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
    )
  )
)

