(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "VOR1060M4T" (in_bom yes) (on_board yes)
    (property "Reference" "K" (at 19.05 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "VOR1060M4T" (at 19.05 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "VOR1060M4T" (at 19.05 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.vishay.com/docs/80406/vor1060m4.pdf" (at 19.05 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Solid State Relays - PCB Mount 1 Form A Solid State Relay SOP-4 Package - Loads up to 600 V" (at 19.05 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "2.38" (at 19.05 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "78-VOR1060M4T" (at 19.05 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Vishay/VOR1060M4T?qs=iLKYxzqNS74u7SR47gH6qg%3D%3D" (at 19.05 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Vishay" (at 19.05 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "VOR1060M4T" (at 19.05 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 17.78 -5.08)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "A" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "K" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 -2.54 180) (length 5.08)
      (name "S2" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 0 180) (length 5.08)
      (name "S1" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
  )
)
