VERSION ""


NS_ : 
	NS_DESC_
	CM_
	BA_DEF_
	BA_
	VAL_
	CAT_DEF_
	CAT_
	FILTER
	BA_DEF_DEF_
	EV_DATA_
	ENVVAR_DATA_
	SGTYPE_
	SGTYPE_VAL_
	BA_DEF_SGTYPE_
	BA_SGTYPE_
	SIG_TYPE_REF_
	VAL_TABLE_
	SIG_GROUP_
	SIG_VALTYPE_
	SIGTYPE_VALTYPE_
	BO_TX_BU_
	BA_DEF_REL_
	BA_REL_
	BA_DEF_DEF_REL_
	BU_SG_REL_
	BU_EV_REL_
	BU_BO_REL_
	SG_MUL_VAL_

BS_:

BU_:


BO_ 3221225472 VECTOR__INDEPENDENT_SIG_MSG: 0 Vector__XXX
 SG_ TTS_TireID_Rear : 0|8@1+ (1,0) [0|255] "" Vector__XXX

BO_ 1792 TTS_Config: 6 Vector__XXX
 SG_ TTS_TireID_Front : 40|8@1+ (1,0) [0|255] "" Vector__XXX
 SG_ TTS_CarID : 32|8@1+ (1,0) [0|255] "" Vector__XXX
 SG_ TTS_Config_epsilon : 16|16@1+ (0.001,0) [0|65.535] "" Vector__XXX
 SG_ TTS_Config_ID : 0|11@1+ (1,0) [0|2047] "" Vector__XXX

BO_ 1796 TTS_RR: 8 Vector__XXX
 SG_ TTS_Status : 60|4@1+ (1,0) [0|15] "" Vector__XXX
 SG_ TTS_OuterRight : 48|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterRight : 36|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_Center : 24|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterLeft : 12|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_OuterLeft : 0|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX

BO_ 1795 TTS_RL: 8 Vector__XXX
 SG_ TTS_Status : 60|4@1+ (1,0) [0|15] "" Vector__XXX
 SG_ TTS_OuterRight : 48|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterRight : 36|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_Center : 24|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterLeft : 12|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_OuterLeft : 0|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX

BO_ 1794 TTS_FR: 8 Vector__XXX
 SG_ TTS_Status : 60|4@1+ (1,0) [0|15] "" Vector__XXX
 SG_ TTS_OuterRight : 48|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterRight : 36|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_Center : 24|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterLeft : 12|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_OuterLeft : 0|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX

BO_ 1793 TTS_FL: 8 Vector__XXX
 SG_ TTS_Status : 60|4@1+ (1,0) [0|15] "" Vector__XXX
 SG_ TTS_OuterRight : 48|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterRight : 36|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_Center : 24|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_CenterLeft : 12|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX
 SG_ TTS_OuterLeft : 0|12@1+ (0.1,0) [0|409.5] "°C" Vector__XXX



CM_ BO_ 3221225472 "This is a message for not used signals, created by Vector CANdb++ DBC OLE DB Provider.";
BA_DEF_  "MultiplexExtEnabled" ENUM  "No","Yes";
BA_DEF_  "BusType" STRING ;
BA_DEF_DEF_  "MultiplexExtEnabled" "No";
BA_DEF_DEF_  "BusType" "CAN";

