(footprint "Micro_Mate-N-Lok_2p_vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 3.81 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "42713045-fffd-4b2d-ae1e-7232d705fb12")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Micro_Mate-N-Lok_2p_vertical"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c0515cd2-cdaa-467e-8354-0f6eadfa35c9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Micro_Mate-N-Lok_2p_vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b898cf0a-05f1-4c3b-be4e-d91efa4940f9")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a88b67c9-ac78-4a8c-859a-d3187554084d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5a17c508-2162-46c6-99ef-5ad462d1b667")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.81 -2.54)
		(end -2.54 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3742a313-c63e-4807-a7bf-be5a0ae2c781")
	)
	(fp_line
		(start -3.81 -1.27)
		(end -3.81 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5e27f565-c85a-4f3b-9862-58c0accdd5e3")
	)
	(fp_line
		(start -3.81 2.54)
		(end -3.81 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d35d7027-ac1b-44b2-9664-3d8a37ee0f4e")
	)
	(fp_line
		(start -3.81 2.54)
		(end 3.81 2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1c052668-6749-425a-9a77-35f046c8aa39")
	)
	(fp_line
		(start -0.508 -3.302)
		(end 0.508 -3.302)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4ba06b66-7669-4c70-b585-f5d4c9c33527")
	)
	(fp_line
		(start 2.54 -2.54)
		(end 3.81 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e8558fbd-ea42-43a6-966a-7bd304bdfaad")
	)
	(fp_line
		(start 3.81 -2.54)
		(end 3.81 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2b894b8a-c098-4d9d-be0f-2ef41dea274e")
	)
	(fp_line
		(start 3.81 2.54)
		(end 3.81 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "25ca9482-069d-43de-b77e-6f2ad77fa017")
	)
	(fp_rect
		(start -7.62 -5.08)
		(end 7.62 2.54)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "312474c5-a081-4cd1-b2e6-730f0718514a")
	)
	(fp_line
		(start 4.318 1.27)
		(end 5.08 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6462399-f2e4-4f1a-b34a-b49a04c8bdb9")
	)
	(fp_line
		(start 4.318 1.778)
		(end 4.318 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1bf544e3-5940-4576-9291-2464e95c0ee2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd roundrect
		(at -5.2 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1f3003e6-dce5-420f-906b-3f1e92b67249")
	)
	(pad "" smd roundrect
		(at 5.2 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "378af8b4-af3d-46e7-89ae-deff12ca9067")
	)
	(pad "1" smd roundrect
		(at -1.5 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ebd06df3-d52b-4cff-99a2-a771df6d3733")
	)
	(pad "2" smd roundrect
		(at 1.5 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "8c0807a7-765b-4fa5-baaa-e09a2b610e6b")
	)
	(model "${KIPRJMOD}/Symbol_Libraries/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_2p_vertical.stp"
		(offset
			(xyz 0 0 9.24)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
