(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "74HC4075" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74HC4075" (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (at 2.54 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd54hc4075.pdf?ts=1705677999042&ref_url=https%253A%252F%252Fwww.google.com%252F" (at 2.54 -25.4 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "TTL Or3" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Triple 3-input OR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74HC4075_1_1"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 4.953)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_1_2"
      (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 0 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_2_1"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 4.953)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 4.318)
        (name "" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_2_2"
      (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 0 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_3_1"
      (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.81 3.81)
          (xy -0.635 3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.635 3.81)
          (xy -3.81 3.81)
          (xy -3.81 3.81)
          (xy -3.556 3.4036)
          (xy -3.0226 2.2606)
          (xy -2.6924 1.0414)
          (xy -2.6162 -0.254)
          (xy -2.7686 -1.4986)
          (xy -3.175 -2.7178)
          (xy -3.81 -3.81)
          (xy -3.81 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 4.953)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_3_2"
      (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at -7.62 0 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_4_0"
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74HC4075_4_1"
      (rectangle (start -5.08 7.62) (end 5.08 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
)
