(footprint "Littelfuse-1350" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 624DBFE7)
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.6 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1eb5b563-08da-43df-964a-cad136b36b3a)
  )
  (fp_text value "Littelfuse-1350" (at 0 4.2 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4ad7d6e2-c100-4878-9a8f-547299f26464)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7ff55e3e-0c1c-4979-bdf8-ff1380ac5586)
  )
  (fp_line (start 7.8 3.4) (end -7.8 3.4) (layer "F.SilkS") (width 0.12) (tstamp 3d5a07a7-d1ad-48b2-ba9a-051332fb8ca3))
  (fp_line (start -7.8 3.4) (end -7.8 -3.4) (layer "F.SilkS") (width 0.12) (tstamp b674899d-e4aa-4f69-aa24-1c3b189f4333))
  (fp_line (start 7.8 -3.4) (end 7.8 3.4) (layer "F.SilkS") (width 0.12) (tstamp d3e28707-f1ad-4ba1-b9a8-d3cdb8de5dcc))
  (fp_line (start -7.8 -3.4) (end 7.8 -3.4) (layer "F.SilkS") (width 0.12) (tstamp ef2838d2-2dc4-4d90-ade9-db000413f63d))
  (fp_line (start -7.6 -3.2) (end 7.6 -3.2) (layer "F.CrtYd") (width 0.05) (tstamp 5e027966-eee4-4c4f-a3fa-9cf52964b0f0))
  (fp_line (start 7.6 3.2) (end -7.6 3.2) (layer "F.CrtYd") (width 0.05) (tstamp 66f10b25-7b1e-4360-8cf3-293a327effef))
  (fp_line (start -7.6 3.2) (end -7.6 -3.2) (layer "F.CrtYd") (width 0.05) (tstamp 8311fa10-f384-4f4d-a23a-dd2982d8b862))
  (fp_line (start 7.6 -3.2) (end 7.6 3.2) (layer "F.CrtYd") (width 0.05) (tstamp eda4cee3-096b-4d8f-9cfe-eb8e507b201e))
  (pad "1" smd rect (at -5.4 0) (size 4 5.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 927d3122-4de3-4e04-b0e1-258d0cc0af01))
  (pad "2" smd rect (at 5.4 0) (size 4 5.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2ca0c609-088e-4b74-b64e-c145dd61f5b0))
)
