PULSONIX_LIBRARY_ASCII "SamacSys ECAD Model"
//960657/1522654/2.50/4/3/Transformer

(asciiHeader
	(fileUnits MM)
)
(library Library_1
	(padStyleDef "r140_80"
		(holeDiam 0)
		(padShape (layerNumRef 1) (padShapeType Rect)  (shapeWidth 0.8) (shapeHeight 1.4))
		(padShape (layerNumRef 16) (padShapeType Ellipse)  (shapeWidth 0) (shapeHeight 0))
	)
	(textStyleDef "Normal"
		(font
			(fontType Stroke)
			(fontFace "Helvetica")
			(fontHeight 1.27)
			(strokeWidth 0.127)
		)
	)
	(patternDef "SOP254P914X350-4N" (originalName "SOP254P914X350-4N")
		(multiLayer
			(pad (padNum 1) (padStyleRef r140_80) (pt -4.325, 1.27) (rotation 90))
			(pad (padNum 2) (padStyleRef r140_80) (pt -4.325, -1.27) (rotation 90))
			(pad (padNum 3) (padStyleRef r140_80) (pt 4.325, -1.27) (rotation 90))
			(pad (padNum 4) (padStyleRef r140_80) (pt 4.325, 1.27) (rotation 90))
		)
		(layerContents (layerNumRef 18)
			(attr "RefDes" "RefDes" (pt 0, 0) (textStyleRef "Normal") (isVisible True))
		)
		(layerContents (layerNumRef Courtyard_Top)
			(line (pt -5.275 2.85) (pt 5.275 2.85) (width 0.05))
		)
		(layerContents (layerNumRef Courtyard_Top)
			(line (pt 5.275 2.85) (pt 5.275 -2.85) (width 0.05))
		)
		(layerContents (layerNumRef Courtyard_Top)
			(line (pt 5.275 -2.85) (pt -5.275 -2.85) (width 0.05))
		)
		(layerContents (layerNumRef Courtyard_Top)
			(line (pt -5.275 -2.85) (pt -5.275 2.85) (width 0.05))
		)
		(layerContents (layerNumRef 28)
			(line (pt -3.55 2.6) (pt 3.55 2.6) (width 0.025))
		)
		(layerContents (layerNumRef 28)
			(line (pt 3.55 2.6) (pt 3.55 -2.6) (width 0.025))
		)
		(layerContents (layerNumRef 28)
			(line (pt 3.55 -2.6) (pt -3.55 -2.6) (width 0.025))
		)
		(layerContents (layerNumRef 28)
			(line (pt -3.55 -2.6) (pt -3.55 2.6) (width 0.025))
		)
		(layerContents (layerNumRef 28)
			(line (pt -3.55 0.06) (pt -1.01 2.6) (width 0.025))
		)
		(layerContents (layerNumRef 18)
			(line (pt -3.275 2.6) (pt 3.275 2.6) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt 3.275 2.6) (pt 3.275 -2.6) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt 3.275 -2.6) (pt -3.275 -2.6) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt -3.275 -2.6) (pt -3.275 2.6) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt -5.025 2.02) (pt -3.625 2.02) (width 0.2))
		)
	)
	(symbolDef "ESMIT-4180_C" (originalName "ESMIT-4180_C")

		(pin (pinNum 1) (pt 0 mils 0 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -25 mils) (rotation 0]) (justify "Left") (textStyleRef "Normal"))
		))
		(pin (pinNum 2) (pt 0 mils -100 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -125 mils) (rotation 0]) (justify "Left") (textStyleRef "Normal"))
		))
		(pin (pinNum 3) (pt 1200 mils 0 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 970 mils -25 mils) (rotation 0]) (justify "Right") (textStyleRef "Normal"))
		))
		(pin (pinNum 4) (pt 1200 mils -100 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 970 mils -125 mils) (rotation 0]) (justify "Right") (textStyleRef "Normal"))
		))
		(line (pt 200 mils 100 mils) (pt 1000 mils 100 mils) (width 6 mils))
		(line (pt 1000 mils 100 mils) (pt 1000 mils -200 mils) (width 6 mils))
		(line (pt 1000 mils -200 mils) (pt 200 mils -200 mils) (width 6 mils))
		(line (pt 200 mils -200 mils) (pt 200 mils 100 mils) (width 6 mils))
		(attr "RefDes" "RefDes" (pt 1050 mils 300 mils) (justify Left) (isVisible True) (textStyleRef "Normal"))
		(attr "Type" "Type" (pt 1050 mils 200 mils) (justify Left) (isVisible True) (textStyleRef "Normal"))

	)
	(compDef "ESMIT-4180_C" (originalName "ESMIT-4180_C") (compHeader (numPins 4) (numParts 1) (refDesPrefix T)
		)
		(compPin "1" (pinName "PRI_1") (partNum 1) (symPinNum 1) (gateEq 0) (pinEq 0) (pinType Unknown))
		(compPin "2" (pinName "PRI_2") (partNum 1) (symPinNum 2) (gateEq 0) (pinEq 0) (pinType Unknown))
		(compPin "4" (pinName "SEC_2") (partNum 1) (symPinNum 3) (gateEq 0) (pinEq 0) (pinType Unknown))
		(compPin "3" (pinName "SEC_1") (partNum 1) (symPinNum 4) (gateEq 0) (pinEq 0) (pinType Unknown))
		(attachedSymbol (partNum 1) (altType Normal) (symbolName "ESMIT-4180_C"))
		(attachedPattern (patternNum 1) (patternName "SOP254P914X350-4N")
			(numPads 4)
			(padPinMap
				(padNum 1) (compPinRef "1")
				(padNum 2) (compPinRef "2")
				(padNum 3) (compPinRef "3")
				(padNum 4) (compPinRef "4")
			)
		)
		(attr "Mouser Part Number" "851-ESMIT-4180/C")
		(attr "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Sumida/ESMIT-4180-C?qs=uFNwyRpLCSIys3VDNoqXHQ%3D%3D")
		(attr "Manufacturer_Name" "Sumida")
		(attr "Manufacturer_Part_Number" "ESMIT-4180/C")
		(attr "Description" "Audio Transformers / Signal Transformers 125uH min 120uH Nom")
		(attr "<Hyperlink>" "http://products.sumida.com/products/pdf/CBM5D33_Ver1.0_E.pdf")
		(attr "<Component Height>" "3.5")
		(attr "<STEP Filename>" "ESMIT-4180_C.stp")
		(attr "<STEP Offsets>" "X=0;Y=0;Z=0")
		(attr "<STEP Rotation>" "X=0;Y=0;Z=0")
	)

)
