(footprint "WCAP-ASLI_16"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -9.4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3cee2c0b-8b35-4535-853d-df8ade17e4aa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WCAP-ASLI_16"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4628875b-f092-48f6-8e44-ec3b9c04543a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4a3e4e95-ebec-48cc-8560-3341d771f0b4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3ad86a96-697c-4d70-af33-70e1c54ba77f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5aaedb51-2641-4bbd-9692-e382e432f052")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -8.1 -8.6)
		(end 6.1 -8.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3f123ee9-28d5-4f79-bcaf-c275979fdb1e")
	)
	(fp_line
		(start -8.1 -1.7)
		(end -8.1 -8.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6c0a3388-d539-414d-bb9e-53a279ec79d6")
	)
	(fp_line
		(start -8.1 1.7)
		(end -8.1 8.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dbcee1c4-42fe-4b03-8b35-37b8775bf28e")
	)
	(fp_line
		(start -8.1 8.6)
		(end 6.1 8.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "64091fe8-2c7f-4b79-903f-43b7efe3e556")
	)
	(fp_line
		(start 6.1 -8.6)
		(end 8.1 -6.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8e8606d6-a6a6-415d-aa0b-d73d31eb7140")
	)
	(fp_line
		(start 6.1 8.6)
		(end 8.1 6.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a8c0d90e-2d70-4413-ab60-2591449a98c1")
	)
	(fp_line
		(start 8.1 -6.6)
		(end 8.1 -1.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "28800248-08d3-44a9-9fd5-8fafd30f651b")
	)
	(fp_line
		(start 8.1 6.6)
		(end 8.1 1.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "af4b0a40-afe6-4cb9-b6ec-d6790150b401")
	)
	(fp_rect
		(start -10 -9.4)
		(end 10 9.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "3f398354-17e2-4891-96bb-d0b72d6e3f85")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e160328d-39ef-438b-a66b-60d815eef80a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at 6.25 0)
		(size 6.5 3.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.12)
		(thermal_bridge_angle 45)
		(uuid "251fa680-5c21-47a1-ac86-de7b148e68fe")
	)
	(pad "2" smd roundrect
		(at -6.25 0)
		(size 6.5 3.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.12)
		(thermal_bridge_angle 45)
		(uuid "cf6b6522-ea88-4837-94cf-95442cfd10d9")
	)
	(model "${KIPRJMOD}/Symbol_Libraries/3DModells/WCAP ASLI 86508xx630xx.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)