(footprint "Micro_Mate-N-Lok_3p_horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -8.25 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "42713045-fffd-4b2d-ae1e-7232d705fb12")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Micro_Mate-N-Lok_3p_horizontal"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c0515cd2-cdaa-467e-8354-0f6eadfa35c9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5b7137ad-53aa-4da5-84c0-0d4e39ccc37a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d1954af9-e372-403e-b95e-35cb9266f88f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cf4eed8f-287d-4bab-8df2-c9aabff6b6e0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.5 1.25)
		(end -5.5 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "908ce94b-b837-4c84-b759-ec4fbb006eea")
	)
	(fp_line
		(start -5.5 -4.5)
		(end -4 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2923d83c-3334-4b85-acfa-e9f2eb6f5eb5")
	)
	(fp_line
		(start -5.5 -1.25)
		(end -6.5 -1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "721eced1-7601-448b-b032-57ae840a5bc6")
	)
	(fp_line
		(start -5.5 -1.25)
		(end -5.5 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "68d14432-223b-47bb-bd26-18873cfb3df2")
	)
	(fp_line
		(start -5.5 1.25)
		(end -5.5 4.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "75ada5c7-eed3-466b-a900-bb7cf3da6f9e")
	)
	(fp_line
		(start -5.5 4.75)
		(end 5.5 4.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d9b138bc-0203-4547-9bd8-5f8e532ba1ac")
	)
	(fp_line
		(start -2 -4.5)
		(end -1 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d0583253-7f1c-498c-afba-93bf9b28c781")
	)
	(fp_line
		(start 1 -4.5)
		(end 2 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "853b4aa5-bf64-4f10-b1c5-492731c47e3b")
	)
	(fp_line
		(start 4 -4.5)
		(end 5.5 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ba3030b2-37eb-4eb2-b7ee-c2f135251592")
	)
	(fp_line
		(start 5.5 -1.25)
		(end 5.5 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f1084b0d-b992-4d4c-9074-1c148a908ad5")
	)
	(fp_line
		(start 5.5 1.25)
		(end 6.5 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8e73e860-7df5-47ee-9d85-a51cffff4073")
	)
	(fp_line
		(start 5.5 4.75)
		(end 5.5 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3836c63d-ca60-4e8e-a339-40980bdccc31")
	)
	(fp_line
		(start 6.5 -1.25)
		(end 5.5 -1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e7987f0c-e4c6-4aae-a5d6-e1cfea057719")
	)
	(fp_circle
		(center 6.25 -5.5)
		(end 6.75 -5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "63489ebf-0f52-43a6-a0ab-158b1a7d4988")
	)
	(fp_rect
		(start -8.5 -7)
		(end 8.5 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "312474c5-a081-4cd1-b2e6-730f0718514a")
	)
	(fp_line
		(start 4.318 1.27)
		(end 5.08 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6462399-f2e4-4f1a-b34a-b49a04c8bdb9")
	)
	(fp_line
		(start 4.318 1.778)
		(end 4.318 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1bf544e3-5940-4576-9291-2464e95c0ee2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd roundrect
		(at -6.7 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1f3003e6-dce5-420f-906b-3f1e92b67249")
	)
	(pad "" smd roundrect
		(at 6.7 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "378af8b4-af3d-46e7-89ae-deff12ca9067")
	)
	(pad "1" smd roundrect
		(at 3 -5.48)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ebd06df3-d52b-4cff-99a2-a771df6d3733")
	)
	(pad "2" smd roundrect
		(at 0 -5.48)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "8c0807a7-765b-4fa5-baaa-e09a2b610e6b")
	)
	(pad "3" smd roundrect
		(at -3 -5.48)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "23e32b5c-4ca6-4614-a426-44d605a7d8fd")
	)
	(model "${KIPRJMOD}/Symbol_Libraries/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_3p_horizontal.stp"
		(offset
			(xyz 0 -4.6 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)