(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "2-1904058-5" (in_bom yes) (on_board yes)
    (property "Reference" "K" (at 21.59 20.32 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "2-1904058-5" (at 21.59 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "219040585" (at 21.59 -82.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=V23700-X0000-A001&DocType=Data%20Sheet&DocLang=English&PartCntxt=2-1904058-5&DocFormat=pdf" (at 21.59 -182.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Body Features: Product Weight .6 OZ | Product Weight 17 G | Contact Features: Contact Arrangement 1 Form X (NO - DM) | Contact Base Material Silver Alloy | Contact Current Class <20 AMP | Dimensions: Product Width .815 INCH | Product Height .76 INCH | Width Class (Mechanical) 20  25 MM | Product Width 20.7 MM | Product Height 19.3 MM | Product Length 1.006 INCH | Length Class (Mechanical) 25  30 MM | Height Class (Mechanical) 16  20 MM | Product Length 25.55 MM | Electrical Characteristics: Insulat" (at 21.59 -282.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "19.6" (at 21.59 -382.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "TE Connectivity" (at 21.59 -482.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "2-1904058-5" (at 21.59 -582.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "571-2-1904058-5" (at 21.59 -682.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity/2-1904058-5/?qs=mU7lhtRCQf7gN3MFkzWqAA%3D%3D" (at 21.59 -782.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "2-1904058-5" (at 21.59 -882.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/2-1904058-5/te-connectivity" (at 21.59 -982.22 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 15.24)
      (end 20.32 -12.7)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 10.16 -17.78 90) (length 5.08)
      (name "COIL+" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 -17.78 90) (length 5.08)
      (name "COIL-" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 -17.78 90) (length 5.08)
      (name "COM" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 20.32 270) (length 5.08)
      (name "OUTPUT+" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 20.32 270) (length 5.08)
      (name "OUTPUT-" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 25.4 0 180) (length 5.08)
      (name "A8" (effects (font (size 1.27 1.27))))
      (number "A8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "B8" (effects (font (size 1.27 1.27))))
      (number "B8" (effects (font (size 1.27 1.27))))
    )
  )
)
