(footprint "Littelfuse_485"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "bb5999d5-f86c-445a-9ff9-2a1b539dc199")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Littelfuse_485"
		(at 0 4.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "8f03ae41-61bd-4463-bc12-db0dde34447c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Littelfuse_485"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b55a18eb-ada8-4ac4-b9cd-3488c889255a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c0dabdc1-ac79-48d9-84bd-8f3d764eb92c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b19461fa-0324-423a-b326-6c3783314d02")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2 -2.5)
		(end 2 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "27ab07ca-24f6-4b98-9e32-937f5364edd2")
	)
	(fp_line
		(start -2 2.5)
		(end 2 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "13f30964-a0e5-4b66-a3b0-82966c8576ce")
	)
	(fp_rect
		(start -7.25 -3.25)
		(end 7.25 3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "d854e56c-a962-466d-bce7-bfb3c9c54498")
	)
	(fp_rect
		(start -6.05 -2.25)
		(end 6.05 2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "3f494321-e87f-4a8e-bbe5-a937d805b012")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b5ea13a8-3e37-4201-b115-0647094f76a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -5.15 0)
		(size 3.5 5.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(uuid "9cb160c0-5456-4bd7-aa7f-b9388d25eb35")
	)
	(pad "2" smd roundrect
		(at 5.15 0)
		(size 3.5 5.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(uuid "9ee66366-9074-4bc0-8447-8c0b7199acdf")
	)
	(model "${KIPRJMOD}/Symbol_Libraries/3DModells/048502.5DR.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
