<?xml version="1.0" encoding="utf-8"?>
<!--/18531122/1522654/2.50/4/2/Switch/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;DIP Switch, Gold Flash Contact Plating, Black, PA9T, 2 Switch, -40  85 C, Extended Actuator, 24 A Contact Rating, Alcoswitch DIP ADE&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ADEN02TTU04">
<description>&lt;b&gt;ADEN02TTU04-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="ADEN02TTU04">
<pin name="1" direction="io"/>
<pin name="2" direction="io"/>
<pin name="3" direction="io"/>
<pin name="4" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADEN02TTU04" prefix="S">
<description>&lt;b&gt;DIP Switch, Gold Flash Contact Plating, Black, PA9T, 2 Switch, -40  85 C, Extended Actuator, 24 A Contact Rating, Alcoswitch DIP ADE&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&amp;DocNm=2454982&amp;DocType=Customer Drawing&amp;DocLang=English&amp;DocFormat=pdf&amp;PartCntxt=2454982-1"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ADEN02TTU04"/>
</gates>
<devices>
<device name="" package="ADEN02TTU04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="Manufacturer_Name" value="TE Connectivity"/>
<attribute name="Manufacturer_Part_Number" value="ADEN02TTU04"/>
<attribute name="Mouser_Part_Number" value="655-ADEN02TTU04"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Alcoswitch/ADEN02TTU04?qs=1Kr7Jg1SGW8ZWHKgHyLd6w%3D%3D"/>
<attribute name="Arrow_Part_Number" value=""/>
<attribute name="Arrow_Price-Stock" value=""/>
<attribute name="Description" value="DIP Switch, Gold Flash Contact Plating, Black, PA9T, 2 Switch, -40  85 C, Extended Actuator, 24 A Contact Rating, Alcoswitch DIP ADE"/>
<attribute name="Height" value="4.51mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
