(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "TPS65105" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 39.37 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS65105" (id 1) (at 0 41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm" (id 2) (at 0 39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps65101.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&ts=1672757737464&ref_url=https%253A%252F%252Fwww.mouser.co.uk%252F" (id 3) (at 0 39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS65105_1_1"
      (rectangle (start -10.16 36.83) (end 8.89 -38.1)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at 11.43 26.67 180) (length 2.54)
        (name "FB1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 11.43 -29.21 180) (length 2.54)
        (name "VCOM" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 15.24 180) (length 2.54)
        (name "VCOMIN" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -21.59 180) (length 2.54)
        (name "FB3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 11.43 -16.51 180) (length 2.54)
        (name "OUT3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 0 0) (length 2.54)
        (name "C2+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
        (name "C2-" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 15.24 0) (length 2.54)
        (name "C1+" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "C1-" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 11.43 8.89 180) (length 2.54)
        (name "DRV" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 1.27 -40.64 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -29.21 0) (length 2.54)
        (name "FB4" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -6.35 180) (length 2.54)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -1.27 180) (length 2.54)
        (name "FB2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 24.13 0) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 27.94 0) (length 2.54)
        (name "ENR" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 30.48 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 3.81 -40.64 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 -21.59 0) (length 2.54)
        (name "BASE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 33.02 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 33.02 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 30.48 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -3.81 -40.64 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -1.27 -40.64 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 22.86 180) (length 2.54)
        (name "SUP" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
