SamacSys ECAD Model
1615215/1031803/2.50/48/3/Integrated Circuit

DESIGNSPARK_INTERMEDIATE_ASCII

(asciiHeader
	(fileUnits MM)
)
(library Library_1
	(padStyleDef "r147.5_30"
		(holeDiam 0)
		(padShape (layerNumRef 1) (padShapeType Rect)  (shapeWidth 0.3) (shapeHeight 1.475))
		(padShape (layerNumRef 16) (padShapeType Ellipse)  (shapeWidth 0) (shapeHeight 0))
	)
	(textStyleDef "Default"
		(font
			(fontType Stroke)
			(fontFace "Helvetica")
			(fontHeight 50 mils)
			(strokeWidth 5 mils)
		)
	)
	(patternDef "QFP50P900X900X160-48N" (originalName "QFP50P900X900X160-48N")
		(multiLayer
			(pad (padNum 1) (padStyleRef r147.5_30) (pt -4.238, 2.75) (rotation 90))
			(pad (padNum 2) (padStyleRef r147.5_30) (pt -4.238, 2.25) (rotation 90))
			(pad (padNum 3) (padStyleRef r147.5_30) (pt -4.238, 1.75) (rotation 90))
			(pad (padNum 4) (padStyleRef r147.5_30) (pt -4.238, 1.25) (rotation 90))
			(pad (padNum 5) (padStyleRef r147.5_30) (pt -4.238, 0.75) (rotation 90))
			(pad (padNum 6) (padStyleRef r147.5_30) (pt -4.238, 0.25) (rotation 90))
			(pad (padNum 7) (padStyleRef r147.5_30) (pt -4.238, -0.25) (rotation 90))
			(pad (padNum 8) (padStyleRef r147.5_30) (pt -4.238, -0.75) (rotation 90))
			(pad (padNum 9) (padStyleRef r147.5_30) (pt -4.238, -1.25) (rotation 90))
			(pad (padNum 10) (padStyleRef r147.5_30) (pt -4.238, -1.75) (rotation 90))
			(pad (padNum 11) (padStyleRef r147.5_30) (pt -4.238, -2.25) (rotation 90))
			(pad (padNum 12) (padStyleRef r147.5_30) (pt -4.238, -2.75) (rotation 90))
			(pad (padNum 13) (padStyleRef r147.5_30) (pt -2.75, -4.238) (rotation 0))
			(pad (padNum 14) (padStyleRef r147.5_30) (pt -2.25, -4.238) (rotation 0))
			(pad (padNum 15) (padStyleRef r147.5_30) (pt -1.75, -4.238) (rotation 0))
			(pad (padNum 16) (padStyleRef r147.5_30) (pt -1.25, -4.238) (rotation 0))
			(pad (padNum 17) (padStyleRef r147.5_30) (pt -0.75, -4.238) (rotation 0))
			(pad (padNum 18) (padStyleRef r147.5_30) (pt -0.25, -4.238) (rotation 0))
			(pad (padNum 19) (padStyleRef r147.5_30) (pt 0.25, -4.238) (rotation 0))
			(pad (padNum 20) (padStyleRef r147.5_30) (pt 0.75, -4.238) (rotation 0))
			(pad (padNum 21) (padStyleRef r147.5_30) (pt 1.25, -4.238) (rotation 0))
			(pad (padNum 22) (padStyleRef r147.5_30) (pt 1.75, -4.238) (rotation 0))
			(pad (padNum 23) (padStyleRef r147.5_30) (pt 2.25, -4.238) (rotation 0))
			(pad (padNum 24) (padStyleRef r147.5_30) (pt 2.75, -4.238) (rotation 0))
			(pad (padNum 25) (padStyleRef r147.5_30) (pt 4.238, -2.75) (rotation 90))
			(pad (padNum 26) (padStyleRef r147.5_30) (pt 4.238, -2.25) (rotation 90))
			(pad (padNum 27) (padStyleRef r147.5_30) (pt 4.238, -1.75) (rotation 90))
			(pad (padNum 28) (padStyleRef r147.5_30) (pt 4.238, -1.25) (rotation 90))
			(pad (padNum 29) (padStyleRef r147.5_30) (pt 4.238, -0.75) (rotation 90))
			(pad (padNum 30) (padStyleRef r147.5_30) (pt 4.238, -0.25) (rotation 90))
			(pad (padNum 31) (padStyleRef r147.5_30) (pt 4.238, 0.25) (rotation 90))
			(pad (padNum 32) (padStyleRef r147.5_30) (pt 4.238, 0.75) (rotation 90))
			(pad (padNum 33) (padStyleRef r147.5_30) (pt 4.238, 1.25) (rotation 90))
			(pad (padNum 34) (padStyleRef r147.5_30) (pt 4.238, 1.75) (rotation 90))
			(pad (padNum 35) (padStyleRef r147.5_30) (pt 4.238, 2.25) (rotation 90))
			(pad (padNum 36) (padStyleRef r147.5_30) (pt 4.238, 2.75) (rotation 90))
			(pad (padNum 37) (padStyleRef r147.5_30) (pt 2.75, 4.238) (rotation 0))
			(pad (padNum 38) (padStyleRef r147.5_30) (pt 2.25, 4.238) (rotation 0))
			(pad (padNum 39) (padStyleRef r147.5_30) (pt 1.75, 4.238) (rotation 0))
			(pad (padNum 40) (padStyleRef r147.5_30) (pt 1.25, 4.238) (rotation 0))
			(pad (padNum 41) (padStyleRef r147.5_30) (pt 0.75, 4.238) (rotation 0))
			(pad (padNum 42) (padStyleRef r147.5_30) (pt 0.25, 4.238) (rotation 0))
			(pad (padNum 43) (padStyleRef r147.5_30) (pt -0.25, 4.238) (rotation 0))
			(pad (padNum 44) (padStyleRef r147.5_30) (pt -0.75, 4.238) (rotation 0))
			(pad (padNum 45) (padStyleRef r147.5_30) (pt -1.25, 4.238) (rotation 0))
			(pad (padNum 46) (padStyleRef r147.5_30) (pt -1.75, 4.238) (rotation 0))
			(pad (padNum 47) (padStyleRef r147.5_30) (pt -2.25, 4.238) (rotation 0))
			(pad (padNum 48) (padStyleRef r147.5_30) (pt -2.75, 4.238) (rotation 0))
		)
		(layerContents (layerNumRef 18)
			(attr "RefDes" "RefDes" (pt 0, 0) (textStyleRef "Default") (isVisible True))
		)
		(layerContents (layerNumRef 30)
			(line (pt -5.225 5.225) (pt 5.225 5.225) (width 0.05))
		)
		(layerContents (layerNumRef 30)
			(line (pt 5.225 5.225) (pt 5.225 -5.225) (width 0.05))
		)
		(layerContents (layerNumRef 30)
			(line (pt 5.225 -5.225) (pt -5.225 -5.225) (width 0.05))
		)
		(layerContents (layerNumRef 30)
			(line (pt -5.225 -5.225) (pt -5.225 5.225) (width 0.05))
		)
		(layerContents (layerNumRef 28)
			(line (pt -3.5 3.5) (pt 3.5 3.5) (width 0.1))
		)
		(layerContents (layerNumRef 28)
			(line (pt 3.5 3.5) (pt 3.5 -3.5) (width 0.1))
		)
		(layerContents (layerNumRef 28)
			(line (pt 3.5 -3.5) (pt -3.5 -3.5) (width 0.1))
		)
		(layerContents (layerNumRef 28)
			(line (pt -3.5 -3.5) (pt -3.5 3.5) (width 0.1))
		)
		(layerContents (layerNumRef 28)
			(line (pt -3.5 3) (pt -3 3.5) (width 0.1))
		)
		(layerContents (layerNumRef 18)
			(line (pt -3.15 3.15) (pt 3.15 3.15) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt 3.15 3.15) (pt 3.15 -3.15) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt 3.15 -3.15) (pt -3.15 -3.15) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt -3.15 -3.15) (pt -3.15 3.15) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(arc (pt -4.725, 3.5) (radius 0.125) (startAngle 0.0) (sweepAngle 0.0) (width 0.25))
		)
		(layerContents (layerNumRef 18)
			(arc (pt -4.725, 3.5) (radius 0.125) (startAngle 180.0) (sweepAngle 180.0) (width 0.25))
		)
	)
	(symbolDef "KSZ8091MLXCA" (originalName "KSZ8091MLXCA")

		(pin (pinNum 1) (pt 0 mils 0 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -25 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 2) (pt 0 mils -100 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -125 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 3) (pt 0 mils -200 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -225 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 4) (pt 0 mils -300 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -325 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 5) (pt 0 mils -400 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -425 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 6) (pt 0 mils -500 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -525 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 7) (pt 0 mils -600 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -625 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 8) (pt 0 mils -700 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -725 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 9) (pt 0 mils -800 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -825 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 10) (pt 0 mils -900 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -925 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 11) (pt 0 mils -1000 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -1025 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 12) (pt 0 mils -1100 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -1125 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 13) (pt 700 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 725 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 14) (pt 800 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 825 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 15) (pt 900 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 925 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 16) (pt 1000 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1025 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 17) (pt 1100 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1125 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 18) (pt 1200 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1225 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 19) (pt 1300 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1325 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 20) (pt 1400 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1425 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 21) (pt 1500 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1525 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 22) (pt 1600 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1625 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 23) (pt 1700 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1725 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 24) (pt 1800 mils -2200 mils) (rotation 90) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1825 mils -1970 mils) (rotation 90]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 25) (pt 2500 mils 0 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -25 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 26) (pt 2500 mils -100 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -125 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 27) (pt 2500 mils -200 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -225 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 28) (pt 2500 mils -300 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -325 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 29) (pt 2500 mils -400 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -425 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 30) (pt 2500 mils -500 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -525 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 31) (pt 2500 mils -600 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -625 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 32) (pt 2500 mils -700 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -725 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 33) (pt 2500 mils -800 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -825 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 34) (pt 2500 mils -900 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -925 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 35) (pt 2500 mils -1000 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -1025 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 36) (pt 2500 mils -1100 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 2270 mils -1125 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 37) (pt 700 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 725 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 38) (pt 800 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 825 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 39) (pt 900 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 925 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 40) (pt 1000 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1025 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 41) (pt 1100 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1125 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 42) (pt 1200 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1225 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 43) (pt 1300 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1325 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 44) (pt 1400 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1425 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 45) (pt 1500 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1525 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 46) (pt 1600 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1625 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 47) (pt 1700 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1725 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 48) (pt 1800 mils 1500 mils) (rotation 270) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 1825 mils 1270 mils) (rotation 90]) (justify "Right") (textStyleRef "Default"))
		))
		(line (pt 200 mils 1300 mils) (pt 2300 mils 1300 mils) (width 6 mils))
		(line (pt 2300 mils 1300 mils) (pt 2300 mils -2000 mils) (width 6 mils))
		(line (pt 2300 mils -2000 mils) (pt 200 mils -2000 mils) (width 6 mils))
		(line (pt 200 mils -2000 mils) (pt 200 mils 1300 mils) (width 6 mils))
		(attr "RefDes" "RefDes" (pt 2350 mils 1500 mils) (justify Left) (isVisible True) (textStyleRef "Default"))

	)
	(compDef "KSZ8091MLXCA" (originalName "KSZ8091MLXCA") (compHeader (numPins 48) (numParts 1) (refDesPrefix IC)
		)
		(compPin "1" (pinName "GND_1") (partNum 1) (symPinNum 1) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "2" (pinName "GND_2") (partNum 1) (symPinNum 2) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "3" (pinName "GND_3") (partNum 1) (symPinNum 3) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "4" (pinName "VDD_1.2_1") (partNum 1) (symPinNum 4) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "5" (pinName "NC_1") (partNum 1) (symPinNum 5) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "6" (pinName "NC_2") (partNum 1) (symPinNum 6) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "7" (pinName "VDDA_3.3") (partNum 1) (symPinNum 7) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "8" (pinName "NC_3") (partNum 1) (symPinNum 8) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "9" (pinName "RXM") (partNum 1) (symPinNum 9) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "10" (pinName "RXP") (partNum 1) (symPinNum 10) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "11" (pinName "TXM") (partNum 1) (symPinNum 11) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "12" (pinName "TXP") (partNum 1) (symPinNum 12) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "13" (pinName "GND_4") (partNum 1) (symPinNum 13) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "14" (pinName "XO") (partNum 1) (symPinNum 14) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "15" (pinName "XI") (partNum 1) (symPinNum 15) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "16" (pinName "REXT") (partNum 1) (symPinNum 16) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "17" (pinName "GND_5") (partNum 1) (symPinNum 17) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "18" (pinName "MDIO") (partNum 1) (symPinNum 18) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "19" (pinName "MDC") (partNum 1) (symPinNum 19) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "20" (pinName "RXD3 / PHYAD0") (partNum 1) (symPinNum 20) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "21" (pinName "RXD2 / PHYAD1") (partNum 1) (symPinNum 21) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "22" (pinName "RXD1 / PHYAD2") (partNum 1) (symPinNum 22) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "23" (pinName "RXD0 / DUPLEX") (partNum 1) (symPinNum 23) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "24" (pinName "GND_6") (partNum 1) (symPinNum 24) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "36" (pinName "TXD1") (partNum 1) (symPinNum 25) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "35" (pinName "TXD0") (partNum 1) (symPinNum 26) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "34" (pinName "TXEN") (partNum 1) (symPinNum 27) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "33" (pinName "TXC / PME_EN") (partNum 1) (symPinNum 28) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "32" (pinName "INTRP / PME_N2 / NAND_TREE#") (partNum 1) (symPinNum 29) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "31" (pinName "VDD_1.2_2") (partNum 1) (symPinNum 30) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "30" (pinName "GND_7") (partNum 1) (symPinNum 31) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "29" (pinName "RXER / ISO") (partNum 1) (symPinNum 32) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "28" (pinName "RXC / B-CAST_OFF") (partNum 1) (symPinNum 33) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "27" (pinName "RXDV / CONFIG2") (partNum 1) (symPinNum 34) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "26" (pinName "NC_4") (partNum 1) (symPinNum 35) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "25" (pinName "VDDIO") (partNum 1) (symPinNum 36) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "48" (pinName "NC_7") (partNum 1) (symPinNum 37) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "47" (pinName "RST#") (partNum 1) (symPinNum 38) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "46" (pinName "NC_6") (partNum 1) (symPinNum 39) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "45" (pinName "NC_5") (partNum 1) (symPinNum 40) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "44" (pinName "TXER") (partNum 1) (symPinNum 41) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "43" (pinName "LED1 / SPEED") (partNum 1) (symPinNum 42) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "42" (pinName "LED0 / PME_N1 / NWAYEN") (partNum 1) (symPinNum 43) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "41" (pinName "CRS / CONFIG1") (partNum 1) (symPinNum 44) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "40" (pinName "COL / CONFIG0") (partNum 1) (symPinNum 45) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "39" (pinName "TXD3") (partNum 1) (symPinNum 46) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "38" (pinName "TXD2") (partNum 1) (symPinNum 47) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "37" (pinName "GND_8") (partNum 1) (symPinNum 48) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(attachedSymbol (partNum 1) (altType Normal) (symbolName "KSZ8091MLXCA"))
		(attachedPattern (patternNum 1) (patternName "QFP50P900X900X160-48N")
			(numPads 48)
			(padPinMap
				(padNum 1) (compPinRef "1")
				(padNum 2) (compPinRef "2")
				(padNum 3) (compPinRef "3")
				(padNum 4) (compPinRef "4")
				(padNum 5) (compPinRef "5")
				(padNum 6) (compPinRef "6")
				(padNum 7) (compPinRef "7")
				(padNum 8) (compPinRef "8")
				(padNum 9) (compPinRef "9")
				(padNum 10) (compPinRef "10")
				(padNum 11) (compPinRef "11")
				(padNum 12) (compPinRef "12")
				(padNum 13) (compPinRef "13")
				(padNum 14) (compPinRef "14")
				(padNum 15) (compPinRef "15")
				(padNum 16) (compPinRef "16")
				(padNum 17) (compPinRef "17")
				(padNum 18) (compPinRef "18")
				(padNum 19) (compPinRef "19")
				(padNum 20) (compPinRef "20")
				(padNum 21) (compPinRef "21")
				(padNum 22) (compPinRef "22")
				(padNum 23) (compPinRef "23")
				(padNum 24) (compPinRef "24")
				(padNum 25) (compPinRef "25")
				(padNum 26) (compPinRef "26")
				(padNum 27) (compPinRef "27")
				(padNum 28) (compPinRef "28")
				(padNum 29) (compPinRef "29")
				(padNum 30) (compPinRef "30")
				(padNum 31) (compPinRef "31")
				(padNum 32) (compPinRef "32")
				(padNum 33) (compPinRef "33")
				(padNum 34) (compPinRef "34")
				(padNum 35) (compPinRef "35")
				(padNum 36) (compPinRef "36")
				(padNum 37) (compPinRef "37")
				(padNum 38) (compPinRef "38")
				(padNum 39) (compPinRef "39")
				(padNum 40) (compPinRef "40")
				(padNum 41) (compPinRef "41")
				(padNum 42) (compPinRef "42")
				(padNum 43) (compPinRef "43")
				(padNum 44) (compPinRef "44")
				(padNum 45) (compPinRef "45")
				(padNum 46) (compPinRef "46")
				(padNum 47) (compPinRef "47")
				(padNum 48) (compPinRef "48")
			)
		)
		(attr "Mouser Part Number" "998-KSZ8091MLXCA")
		(attr "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Microchip-Technology/KSZ8091MLXCA?qs=eR3IRSQlCypqsIaneAp%2FkQ%3D%3D")
		(attr "Manufacturer_Name" "Microchip")
		(attr "Manufacturer_Part_Number" "KSZ8091MLXCA")
		(attr "Description" "Ethernet ICs 10Base-T/100Base PhysLayerTrnscvr")
		(attr "Datasheet Link" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002297A.pdf")
		(attr "Height" "1.6 mm")
	)

)
