(footprint "L_CommonMode_Wuerth_WE-SL2"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "http://katalog.we-online.de/en/pbs/WE-SL2?sid=5fbec16187#vs_t1:c1_ct:1")
	(tags "Wuerth WE-SL2")
	(property "Reference" "REF**"
		(at 0 -4.2 0)
		(layer "F.SilkS")
		(uuid "2368f75b-64df-4ae0-88ef-3447bb8cb9c9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "L_CommonMode_Wuerth_WE-SL2"
		(at 0.4 4.2 0)
		(layer "F.Fab")
		(uuid "00b4d232-1b69-4939-9204-1bde14716cbb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2f9e6410-b468-49c0-bd13-e583b4d1406e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3177f2aa-6ccd-4c51-b494-c0eb50659ab1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "54091877-59ad-4253-bf58-262995836d56")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center 0 0)
		(end 0.5 0)
		(stroke
			(width 1)
			(type solid)
		)
		(fill none)
		(layer "F.Adhes")
		(uuid "190043e3-ef70-4919-a259-1e62b9547cbc")
	)
	(fp_line
		(start -4.9 -2.2)
		(end -4.8 -2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f1efb53f-ba01-4c38-b89a-408a4faa69fa")
	)
	(fp_line
		(start -4.9 -0.3)
		(end -4.7 -0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8d0d4ac1-20d6-4f2d-9729-8690fee3393a")
	)
	(fp_line
		(start -4.7 -3.1)
		(end -4.7 -2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ce48f513-e69d-4459-8db3-638ac1c49cb7")
	)
	(fp_line
		(start -4.7 -3.1)
		(end 4.7 -3.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fecf49f4-5865-42f3-a09b-d46ff2a207b4")
	)
	(fp_line
		(start -4.7 -2.2)
		(end -4.9 -2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "122e0993-224c-40ec-a4ed-86faaba293c7")
	)
	(fp_line
		(start -4.7 -0.3)
		(end -4.7 0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f9e22fea-50af-4664-837d-17418c6fa017")
	)
	(fp_line
		(start -4.7 3.1)
		(end -4.7 2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e9548011-4b1b-4646-84eb-4e3c880ad279")
	)
	(fp_line
		(start 4.7 -3.1)
		(end 4.7 -2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9d0b1688-bf94-4d1d-a136-8161644eb6fd")
	)
	(fp_line
		(start 4.7 -0.3)
		(end 4.7 0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b8c799bc-3ff8-4ef1-ab17-664a341d5a8f")
	)
	(fp_line
		(start 4.7 3.1)
		(end -4.7 3.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "899afbe1-ff97-47a5-9f28-3860bfbc2186")
	)
	(fp_line
		(start 4.7 3.1)
		(end 4.7 2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "17f7d24f-2153-42e0-9e8d-33cdb0165c09")
	)
	(fp_line
		(start -5 -3.25)
		(end 5 -3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3d609d96-ae1d-4816-bd4d-e3c97f084c52")
	)
	(fp_line
		(start -5 3.25)
		(end -5 -3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "251c4a56-095c-40aa-9c32-4383f86839a0")
	)
	(fp_line
		(start 5 -3.25)
		(end 5 3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4c894634-e418-4bd4-a106-a1d43bfbe886")
	)
	(fp_line
		(start 5 3.25)
		(end -5 3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7c52530e-91ac-458f-b176-7c139f6da467")
	)
	(fp_line
		(start -4.6 -2.9)
		(end -4.5 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5e716446-ea64-4e3e-89a0-c2f8e5762d4c")
	)
	(fp_line
		(start -4.6 -2.2)
		(end -3.8 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "63c06f5a-3c7e-4907-b88d-257d0cbb60bb")
	)
	(fp_line
		(start -4.6 -2)
		(end -4.6 -2.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "24d7a864-33f2-473d-b0bf-a64e290b0502")
	)
	(fp_line
		(start -4.6 -2)
		(end -4.6 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2fec4337-48e0-4add-bf20-bc807838bb21")
	)
	(fp_line
		(start -4.5 -3)
		(end -3.6 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c88aef9a-490f-4353-b74c-e82667574108")
	)
	(fp_line
		(start -3.6 -3)
		(end 4.6 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dbf34498-4c54-4ed4-8fbb-8c8b12040cdc")
	)
	(fp_line
		(start 4.6 -3)
		(end 4.6 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d47e5616-9e86-47cd-9ad2-a849d35a0d6e")
	)
	(fp_line
		(start 4.6 3)
		(end -4.6 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "03e87013-dd29-403f-90a4-c47ae9d65a7a")
	)
	(fp_text user "${REFERENCE}"
		(at -0.02 0 0)
		(layer "F.Fab")
		(uuid "de54dfef-811d-4b3b-8f2a-101d1455a227")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -3.75 -1.27)
		(size 2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "d068672e-48ef-4feb-9ec7-c3630de76bdc")
	)
	(pad "2" smd rect
		(at -3.75 1.27)
		(size 2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f8a31fce-e626-4c77-94ce-c4213151f77c")
	)
	(pad "3" smd rect
		(at 3.75 1.27)
		(size 2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "c6dc3aa4-cf14-4ed0-af6c-03f348f44fae")
	)
	(pad "4" smd rect
		(at 3.75 -1.27)
		(size 2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "e27df121-02e8-4749-bcdf-a7eb946387d6")
	)
	(model "${KIPRJMOD}/KiCAD_lib/stp/WE-SL2_74422 (rev1).stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)