FILE_TYPE = MULTI_PHYS_TABLE;

PART 'SN75LVDS83BDGGR'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Texas Instruments", "SN75LVDS83BDGGR" (!) = "", "SOP50P810X120-56N", "Small Outline Packages", "595-SN75LVDS83BDGGR", "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/SN75LVDS83BDGGR?qs=IDSsxkoac0yg4KfFeU4liA%3D%3D", "10- to 135-MHz 28-bit LVDS transmitter/serializer & FlatLink integrated circuit", "https://www.ti.com/lit/gpn/SN75LVDS83B", "1.2 mm"
END_PART

END.
