(footprint "JST_GH_THT_1x06-1MP_P1.25mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "JST GH series connector, BM06B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST GH vertical")
	(property "Reference" "REF**"
		(at 1.75 -2.5 0)
		(layer "F.SilkS")
		(uuid "31c9bf08-ba70-4a44-8a71-2e285dd7aa12")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "JST_GH_THT_1x06-1MP_P1.25mm_Vertical"
		(at 3.375 4.25 0)
		(layer "F.Fab")
		(uuid "794d0921-bc5d-42c8-b2ef-4022fbe52d43")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 3.375 0.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2276f8b5-1629-4a3a-8bc8-e50b396a5886")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 3.375 0.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e7f5aa4c-acdd-4de4-9ee3-1fd5f407d140")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 3.375 0.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ad93baf2-6bd9-4bf9-afea-fcd68a58104b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.5 0.51)
		(end -1.5 2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5a0afb6c-9778-4692-9739-ddd9a5cb63a9")
	)
	(fp_line
		(start -1.5 2.2)
		(end 0.25 2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "40bc8190-c038-4e59-8327-e7f04c05f3c1")
	)
	(fp_line
		(start -0.84 -1.05)
		(end 7.59 -1.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ab3a667d-8af4-4f10-a15b-b360ab502ea8")
	)
	(fp_line
		(start 0.25 2.2)
		(end 0.25 3.17)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "75b78d20-1b8c-4c77-a109-aa7e7549ab11")
	)
	(fp_line
		(start 8.25 0.51)
		(end 8.25 2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b2e4a647-0542-4838-9eda-758f79f71cb9")
	)
	(fp_line
		(start 8.25 2.2)
		(end 6.45 2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "15b973f1-df57-41e5-b3a7-0b172f4dceed")
	)
	(fp_rect
		(start -2 -1.55)
		(end 8.75 2.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "6d837f48-a7f3-40e9-ad83-64a3ffad8fae")
	)
	(fp_line
		(start -0.25 2.2)
		(end 0.25 1.492893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e219b7b8-2faf-4a47-8f72-c1130643d842")
	)
	(fp_line
		(start 0 -0.25)
		(end 0 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fbf901d5-6aba-4422-b48d-19b76d0fd43c")
	)
	(fp_line
		(start 0 0.25)
		(end 0.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dff7d06e-a324-4db3-ae82-f1bc3d9874b5")
	)
	(fp_line
		(start 0.25 1.492893)
		(end 0.75 2.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8de2cf49-8c73-46ab-9422-758c94833a3a")
	)
	(fp_line
		(start 0.5 -0.25)
		(end 0 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9df11798-b935-4ac9-b2d7-052a4af21768")
	)
	(fp_line
		(start 0.5 0.25)
		(end 0.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "107611d3-34bb-4521-a883-6cfa5338d7d7")
	)
	(fp_line
		(start 1.25 -0.25)
		(end 1.25 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "212de075-d5a0-48eb-bde4-6240457fc21d")
	)
	(fp_line
		(start 1.25 0.25)
		(end 1.75 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cf4cf8a9-7f07-4300-8f78-748f486012a6")
	)
	(fp_line
		(start 1.75 -0.25)
		(end 1.25 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "eaf6b2d6-70ae-4ada-a60f-dc3fb7fcd2ae")
	)
	(fp_line
		(start 1.75 0.25)
		(end 1.75 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b245ebbd-3c96-45b6-9816-94376be85930")
	)
	(fp_line
		(start 2.5 -0.25)
		(end 2.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "33b08e44-41b3-4c8b-88e9-2e9024d0ecca")
	)
	(fp_line
		(start 2.5 0.25)
		(end 3 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b644d55a-e9f5-4ffb-b45f-63a0f1b538d2")
	)
	(fp_line
		(start 3 -0.25)
		(end 2.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4aa827f5-1c2f-4d97-919c-f3a4652caa31")
	)
	(fp_line
		(start 3 0.25)
		(end 3 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7e62f849-461a-4263-bd50-ecefcafc51f4")
	)
	(fp_line
		(start 3.75 -0.25)
		(end 3.75 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "85ea2f3a-c503-4361-a1c5-f7d2f23eb0b5")
	)
	(fp_line
		(start 3.75 0.25)
		(end 4.25 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4eeae548-3b9f-426e-940d-1b9f554bd763")
	)
	(fp_line
		(start 4.25 -0.25)
		(end 3.75 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3c462c2b-0b15-499e-9a27-2afb132638d7")
	)
	(fp_line
		(start 4.25 0.25)
		(end 4.25 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "02b6232a-83d5-41c9-a9b2-189895bffd34")
	)
	(fp_line
		(start 5 -0.25)
		(end 5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3aaea4a4-842d-4167-9211-6c098c4954b1")
	)
	(fp_line
		(start 5 0.25)
		(end 5.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1a0f3bc1-0859-4e18-a59b-29b5f7c6ea78")
	)
	(fp_line
		(start 5.5 -0.25)
		(end 5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2abff4d4-0140-4b27-b717-9d79f695d8b4")
	)
	(fp_line
		(start 5.5 0.25)
		(end 5.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b96a4b8b-ba97-46f9-812e-cebb114b49de")
	)
	(fp_line
		(start 6.25 -0.25)
		(end 6.25 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "52f4a742-51b8-4651-ac89-a71ceb779d77")
	)
	(fp_line
		(start 6.25 0.25)
		(end 6.75 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5beef47b-b319-4489-906b-50d9de1242b4")
	)
	(fp_line
		(start 6.75 -0.25)
		(end 6.25 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fcf6adf4-a742-42a1-804f-b1acbe3b09b5")
	)
	(fp_line
		(start 6.75 0.25)
		(end 6.75 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "776d0ba7-2faf-4812-acc1-b5f15f076357")
	)
	(fp_rect
		(start -1.5 -1.05)
		(end 8.25 2.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "f6da2cea-ffbd-44b8-be42-ef29eb49ba6c")
	)
	(fp_text user "${REFERENCE}"
		(at 3.375 -1.25 0)
		(layer "F.Fab")
		(uuid "1d3419ec-398e-4b1b-8d93-297bc83d9799")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0.25 -0.05)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "edee433e-7c84-4e6c-bdaa-e573378e45b3")
	)
	(pad "2" thru_hole circle
		(at 1.5 -0.05)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8b4bb553-fa48-4857-bb8e-2ffaa745e103")
	)
	(pad "3" thru_hole circle
		(at 2.75 -0.05)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8b387d51-079a-4b18-a6fb-94572759e09c")
	)
	(pad "4" thru_hole circle
		(at 4 -0.05)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0c1df370-ad86-4d07-aee0-ecc391bd7514")
	)
	(pad "5" thru_hole circle
		(at 5.25 -0.05)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bb152250-41c6-415c-9ddf-62701c213950")
	)
	(pad "6" thru_hole circle
		(at 6.5 -0.05)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c4a10b04-a17c-4546-8bc8-b046618b2035")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM06B-GHS-TBT_1x06-1MP_P1.25mm_Vertical.wrl"
		(offset
			(xyz 3.5 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
