{
  "board": {
    "3dviewports": [],
    "design_settings": {
      "defaults": {
        "apply_defaults_to_fp_fields": false,
        "apply_defaults_to_fp_shapes": false,
        "apply_defaults_to_fp_text": false,
        "board_outline_line_width": 0.1,
        "copper_line_width": 0.2,
        "copper_text_italic": false,
        "copper_text_size_h": 1.5,
        "copper_text_size_v": 1.5,
        "copper_text_thickness": 0.3,
        "copper_text_upright": false,
        "courtyard_line_width": 0.05,
        "dimension_precision": 4,
        "dimension_units": 3,
        "dimensions": {
          "arrow_length": 1270000,
          "extension_offset": 500000,
          "keep_text_aligned": true,
          "suppress_zeroes": false,
          "text_position": 0,
          "units_format": 1
        },
        "fab_line_width": 0.1,
        "fab_text_italic": false,
        "fab_text_size_h": 1.0,
        "fab_text_size_v": 1.0,
        "fab_text_thickness": 0.15,
        "fab_text_upright": false,
        "other_line_width": 0.15,
        "other_text_italic": false,
        "other_text_size_h": 1.0,
        "other_text_size_v": 1.0,
        "other_text_thickness": 0.15,
        "other_text_upright": false,
        "pads": {
          "drill": 2.0,
          "height": 2.0,
          "width": 2.0
        },
        "silk_line_width": 0.15,
        "silk_text_italic": false,
        "silk_text_size_h": 1.0,
        "silk_text_size_v": 1.0,
        "silk_text_thickness": 0.15,
        "silk_text_upright": false,
        "zones": {
          "min_clearance": 0.2
        }
      },
      "diff_pair_dimensions": [
        {
          "gap": 0.0,
          "via_gap": 0.0,
          "width": 0.0
        }
      ],
      "drc_exclusions": [],
      "meta": {
        "version": 2
      },
      "rule_severities": {
        "annular_width": "error",
        "clearance": "error",
        "connection_width": "warning",
        "copper_edge_clearance": "error",
        "copper_sliver": "warning",
        "courtyards_overlap": "error",
        "diff_pair_gap_out_of_range": "error",
        "diff_pair_uncoupled_length_too_long": "error",
        "drill_out_of_range": "error",
        "duplicate_footprints": "warning",
        "extra_footprint": "warning",
        "footprint": "error",
        "footprint_symbol_mismatch": "warning",
        "footprint_type_mismatch": "warning",
        "hole_clearance": "error",
        "hole_near_hole": "error",
        "holes_co_located": "warning",
        "invalid_outline": "error",
        "isolated_copper": "warning",
        "item_on_disabled_layer": "error",
        "items_not_allowed": "error",
        "length_out_of_range": "error",
        "lib_footprint_issues": "warning",
        "lib_footprint_mismatch": "ignore",
        "malformed_courtyard": "error",
        "microvia_drill_out_of_range": "error",
        "missing_courtyard": "ignore",
        "missing_footprint": "warning",
        "net_conflict": "warning",
        "npth_inside_courtyard": "ignore",
        "padstack": "warning",
        "pth_inside_courtyard": "ignore",
        "shorting_items": "error",
        "silk_edge_clearance": "warning",
        "silk_over_copper": "warning",
        "silk_overlap": "warning",
        "skew_out_of_range": "error",
        "solder_mask_bridge": "error",
        "starved_thermal": "error",
        "text_height": "warning",
        "text_thickness": "warning",
        "through_hole_pad_without_hole": "error",
        "too_many_vias": "error",
        "track_dangling": "warning",
        "track_width": "error",
        "tracks_crossing": "error",
        "unconnected_items": "error",
        "unresolved_variable": "error",
        "via_dangling": "warning",
        "zones_intersect": "error"
      },
      "rules": {
        "max_error": 0.005,
        "min_clearance": 0.0,
        "min_connection": 0.0,
        "min_copper_edge_clearance": 0.3,
        "min_hole_clearance": 0.25,
        "min_hole_to_hole": 0.25,
        "min_microvia_diameter": 0.2,
        "min_microvia_drill": 0.1,
        "min_resolved_spokes": 1,
        "min_silk_clearance": 0.0,
        "min_text_height": 0.8,
        "min_text_thickness": 0.08,
        "min_through_hole_diameter": 0.3,
        "min_track_width": 0.0,
        "min_via_annular_width": 0.1,
        "min_via_diameter": 0.5,
        "solder_mask_clearance": 0.0,
        "solder_mask_min_width": 0.0,
        "solder_mask_to_copper_clearance": 0.0,
        "use_height_for_length_calcs": true
      },
      "teardrop_options": [
        {
          "td_onpadsmd": true,
          "td_onroundshapesonly": false,
          "td_ontrackend": false,
          "td_onviapad": true
        }
      ],
      "teardrop_parameters": [
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_round_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_rect_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_track_end",
          "td_width_to_size_filter_ratio": 0.9
        }
      ],
      "track_widths": [
        0.0,
        0.15,
        0.2,
        0.3,
        0.5,
        1.0
      ],
      "tuning_pattern_settings": {
        "diff_pair_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 1.0
        },
        "diff_pair_skew_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        },
        "single_track_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        }
      },
      "via_dimensions": [
        {
          "diameter": 0.0,
          "drill": 0.0
        }
      ],
      "zones_allow_external_fillets": false
    },
    "ipc2581": {
      "dist": "",
      "distpn": "",
      "internal_id": "",
      "mfg": "",
      "mpn": ""
    },
    "layer_presets": [],
    "viewports": []
  },
  "boards": [],
  "cvpcb": {
    "equivalence_files": []
  },
  "erc": {
    "erc_exclusions": [],
    "meta": {
      "version": 0
    },
    "pin_map": [
      [
        0,
        0,
        0,
        0,
        0,
        0,
        1,
        0,
        0,
        0,
        0,
        2
      ],
      [
        0,
        2,
        0,
        1,
        0,
        0,
        1,
        0,
        2,
        2,
        2,
        2
      ],
      [
        0,
        0,
        0,
        0,
        0,
        0,
        1,
        0,
        1,
        0,
        1,
        2
      ],
      [
        0,
        1,
        0,
        0,
        0,
        0,
        1,
        1,
        2,
        1,
        1,
        2
      ],
      [
        0,
        0,
        0,
        0,
        0,
        0,
        1,
        0,
        0,
        0,
        0,
        2
      ],
      [
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        2
      ],
      [
        1,
        1,
        1,
        1,
        1,
        0,
        1,
        1,
        1,
        1,
        1,
        2
      ],
      [
        0,
        0,
        0,
        1,
        0,
        0,
        1,
        0,
        0,
        0,
        0,
        2
      ],
      [
        0,
        2,
        1,
        2,
        0,
        0,
        1,
        0,
        2,
        2,
        2,
        2
      ],
      [
        0,
        2,
        0,
        1,
        0,
        0,
        1,
        0,
        2,
        0,
        0,
        2
      ],
      [
        0,
        2,
        1,
        1,
        0,
        0,
        1,
        0,
        2,
        0,
        0,
        2
      ],
      [
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2
      ]
    ],
    "rule_severities": {
      "bus_definition_conflict": "error",
      "bus_entry_needed": "error",
      "bus_to_bus_conflict": "error",
      "bus_to_net_conflict": "error",
      "conflicting_netclasses": "error",
      "different_unit_footprint": "error",
      "different_unit_net": "error",
      "duplicate_reference": "error",
      "duplicate_sheet_names": "error",
      "endpoint_off_grid": "ignore",
      "extra_units": "error",
      "global_label_dangling": "warning",
      "hier_label_mismatch": "error",
      "label_dangling": "error",
      "lib_symbol_issues": "ignore",
      "missing_bidi_pin": "warning",
      "missing_input_pin": "warning",
      "missing_power_pin": "error",
      "missing_unit": "warning",
      "multiple_net_names": "warning",
      "net_not_bus_member": "warning",
      "no_connect_connected": "warning",
      "no_connect_dangling": "warning",
      "pin_not_connected": "error",
      "pin_not_driven": "error",
      "pin_to_pin": "error",
      "power_pin_not_driven": "error",
      "similar_labels": "warning",
      "simulation_model_issue": "ignore",
      "unannotated": "error",
      "unit_value_mismatch": "error",
      "unresolved_variable": "error",
      "wire_dangling": "error"
    }
  },
  "libraries": {
    "pinned_footprint_libs": [],
    "pinned_symbol_libs": []
  },
  "meta": {
    "filename": "PDU FT24.kicad_pro",
    "version": 1
  },
  "net_settings": {
    "classes": [
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.25,
        "via_diameter": 0.8,
        "via_drill": 0.4,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "10A_Power",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgb(246, 190, 0)",
        "track_width": 0.25,
        "via_diameter": 0.8,
        "via_drill": 0.4,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "20A_Power",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgb(246, 190, 0)",
        "track_width": 0.25,
        "via_diameter": 0.8,
        "via_drill": 0.4,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "5A_Power",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgb(246, 190, 0)",
        "track_width": 0.25,
        "via_diameter": 0.8,
        "via_drill": 0.4,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Analog",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgb(255, 0, 241)",
        "track_width": 0.25,
        "via_diameter": 0.8,
        "via_drill": 0.4,
        "wire_width": 6
      }
    ],
    "meta": {
      "version": 3
    },
    "net_colors": null,
    "netclass_assignments": {
      "/Connectors/POut12": "7.5A_Power",
      "/Connectors/POut13": "7.5A_Power",
      "/Connectors/POut18": "20A_Power",
      "/Connectors/POut19": "20A_Power",
      "/Connectors/POut2": "5A_Power",
      "/Connectors/POut4": "5A_Power",
      "/Connectors/POut5": "5A_Power",
      "/Connectors/POut6": "5A_Power",
      "/Connectors/POut7": "5A_Power",
      "/Power Stages/IS1": "Analog",
      "/Power Stages/IS10": "Analog",
      "/Power Stages/IS11": "Analog",
      "/Power Stages/IS12": "Analog",
      "/Power Stages/IS13": "Analog",
      "/Power Stages/IS2": "Analog",
      "/Power Stages/IS3": "Analog",
      "/Power Stages/IS4": "Analog",
      "/Power Stages/IS5": "Analog",
      "/Power Stages/IS6": "Analog",
      "/Power Stages/IS7": "Analog",
      "/Power Stages/IS9": "Analog",
      "12V_EBS_Relay": "5A_Power",
      "Net-(D13-K)": "Analog",
      "Net-(D14-K)": "Analog",
      "Net-(D20-K)": "Analog",
      "Net-(D38-K)": "Analog",
      "Net-(D41-K)": "Analog",
      "Net-(D47-K)": "Analog",
      "Net-(D56-K)": "Analog",
      "Net-(D58-K)": "Analog",
      "Net-(D6-K)": "Analog",
      "Net-(D60-K)": "Analog",
      "Net-(D62-K)": "Analog",
      "Net-(D9-K)": "Analog",
      "Net-(IC10-IS)": "Analog",
      "Net-(IC9-IS)": "Analog",
      "Net-(U10-IS)": "Analog",
      "Net-(U10-VS)": "5A_Power",
      "Net-(U11-IS)": "Analog",
      "Net-(U18-IS)": "Analog",
      "Net-(U32-IS)": "Analog",
      "Net-(U32-VS)": "10A_Power",
      "Net-(U36-IS)": "Analog",
      "Net-(U44-IS)": "Analog",
      "Net-(U46-IS)": "Analog",
      "Net-(U48-IS)": "Analog",
      "Net-(U50-IS)": "Analog",
      "Net-(U7-IS)": "Analog",
      "Net-(U9-IS)": "Analog",
      "Net-(U9-VS)": "10A_Power"
    },
    "netclass_patterns": []
  },
  "pcbnew": {
    "last_paths": {
      "gencad": "",
      "idf": "",
      "netlist": "",
      "plot": "gerber export/",
      "pos_files": "",
      "specctra_dsn": "",
      "step": "../../../PDU FT24 v10.1 STEP export.step",
      "svg": "",
      "vrml": ""
    },
    "page_layout_descr_file": ""
  },
  "schematic": {
    "annotate_start_num": 0,
    "bom_export_filename": "",
    "bom_fmt_presets": [],
    "bom_fmt_settings": {
      "field_delimiter": ",",
      "keep_line_breaks": false,
      "keep_tabs": false,
      "name": "CSV",
      "ref_delimiter": ",",
      "ref_range_delimiter": "",
      "string_delimiter": "\""
    },
    "bom_presets": [],
    "bom_settings": {
      "exclude_dnp": false,
      "fields_ordered": [
        {
          "group_by": false,
          "label": "Reference",
          "name": "Reference",
          "show": true
        },
        {
          "group_by": true,
          "label": "Value",
          "name": "Value",
          "show": true
        },
        {
          "group_by": false,
          "label": "Datasheet",
          "name": "Datasheet",
          "show": true
        },
        {
          "group_by": false,
          "label": "Footprint",
          "name": "Footprint",
          "show": true
        },
        {
          "group_by": false,
          "label": "Qty",
          "name": "${QUANTITY}",
          "show": true
        },
        {
          "group_by": true,
          "label": "DNP",
          "name": "${DNP}",
          "show": true
        },
        {
          "group_by": false,
          "label": "#",
          "name": "${ITEM_NUMBER}",
          "show": false
        },
        {
          "group_by": false,
          "label": "Arrow Part Number",
          "name": "Arrow Part Number",
          "show": false
        },
        {
          "group_by": false,
          "label": "Arrow Price/Stock",
          "name": "Arrow Price/Stock",
          "show": false
        },
        {
          "group_by": false,
          "label": "Height",
          "name": "Height",
          "show": false
        },
        {
          "group_by": false,
          "label": "Manufacturer_Name",
          "name": "Manufacturer_Name",
          "show": false
        },
        {
          "group_by": false,
          "label": "Manufacturer_Part_Number",
          "name": "Manufacturer_Part_Number",
          "show": false
        },
        {
          "group_by": false,
          "label": "Mouser Part Number",
          "name": "Mouser Part Number",
          "show": false
        },
        {
          "group_by": false,
          "label": "Mouser Price/Stock",
          "name": "Mouser Price/Stock",
          "show": false
        },
        {
          "group_by": false,
          "label": "Sim.Device",
          "name": "Sim.Device",
          "show": false
        },
        {
          "group_by": false,
          "label": "Sim.Pins",
          "name": "Sim.Pins",
          "show": false
        },
        {
          "group_by": false,
          "label": "heisener Part Number",
          "name": "heisener Part Number",
          "show": false
        },
        {
          "group_by": false,
          "label": "heisener Price/Stock",
          "name": "heisener Price/Stock",
          "show": false
        },
        {
          "group_by": false,
          "label": "Description",
          "name": "Description",
          "show": false
        }
      ],
      "filter_string": "",
      "group_symbols": true,
      "name": "",
      "sort_asc": true,
      "sort_field": "Reference"
    },
    "connection_grid_size": 50.0,
    "drawing": {
      "dashed_lines_dash_length_ratio": 12.0,
      "dashed_lines_gap_length_ratio": 3.0,
      "default_line_thickness": 6.0,
      "default_text_size": 50.0,
      "field_names": [],
      "intersheets_ref_own_page": false,
      "intersheets_ref_prefix": "",
      "intersheets_ref_short": false,
      "intersheets_ref_show": false,
      "intersheets_ref_suffix": "",
      "junction_size_choice": 3,
      "label_size_ratio": 0.375,
      "operating_point_overlay_i_precision": 3,
      "operating_point_overlay_i_range": "~A",
      "operating_point_overlay_v_precision": 3,
      "operating_point_overlay_v_range": "~V",
      "overbar_offset_ratio": 1.23,
      "pin_symbol_size": 25.0,
      "text_offset_ratio": 0.15
    },
    "legacy_lib_dir": "",
    "legacy_lib_list": [],
    "meta": {
      "version": 1
    },
    "net_format_name": "",
    "ngspice": {
      "fix_include_paths": true,
      "meta": {
        "version": 0
      },
      "model_mode": 4,
      "workbook_filename": ""
    },
    "page_layout_descr_file": "",
    "plot_directory": "",
    "spice_current_sheet_as_root": false,
    "spice_external_command": "spice \"%I\"",
    "spice_model_current_sheet_as_root": true,
    "spice_save_all_currents": false,
    "spice_save_all_dissipations": false,
    "spice_save_all_voltages": false,
    "subpart_first_id": 65,
    "subpart_id_separator": 0
  },
  "sheets": [
    [
      "cba93115-b7ba-40c8-a438-b74eea4adf4d",
      "Root"
    ],
    [
      "4e25c724-8f65-40d5-9aed-21011dd956f3",
      "Connectors"
    ],
    [
      "10dbcd3d-c2df-41dc-832d-4c9bd84254e3",
      "MCU"
    ],
    [
      "fc136761-7437-4777-9313-169871d18382",
      "Power Stages"
    ],
    [
      "27ff76aa-7f65-49fe-8358-3575a2f29ca5",
      "Power Supply"
    ],
    [
      "a95c2791-2bc4-47a0-a196-92c226b6c1db",
      "EBS CS Valve "
    ],
    [
      "8b3cc2cc-a42b-46a5-84c4-fd80d916ae87",
      "EBS Valve 1-2"
    ],
    [
      "07ea260a-3d87-40b3-a394-04e99c6e70c5",
      "Always On - SDC"
    ],
    [
      "a30c1bf3-b94f-4d36-b7ea-f869b2d928ef",
      "Misc - Inverter "
    ],
    [
      "7178aaa1-419b-45f4-88fe-7c1d19ced9bd",
      "Pump MotInv 2x7.5A"
    ],
    [
      "43ba33b5-35ed-4409-8523-7daab12cceea",
      "Lidar x Groundspeed GSS 2x7.5A"
    ],
    [
      "a53cc0be-b200-4aeb-9459-d423ea8fc2eb",
      "ACU 1x30A"
    ],
    [
      "c5746397-87b1-42da-896b-86720deb4602",
      "Fans Radiator MotInv ( PWM ) 1x20A"
    ],
    [
      "f9d0761c-a7fc-487d-9cd5-06f6ee74a55b",
      "Fan Acc ( PWM ) 1x30A"
    ],
    [
      "fd18a62a-2d4e-4ad0-824c-b600b1499537",
      "Servos 1x20A"
    ],
    [
      "f7f08656-46b5-4833-87d1-b4bc1c9b11f6",
      "Aggregate ( PWM ) 1x20A"
    ],
    [
      "b093302c-432b-4c9a-ac34-d87497ff35ab",
      "EPSC 1x20A"
    ]
  ],
  "text_variables": {}
}
