;Proteus Design Interchange Format
(PDIF
 (vendor "SamacSys Limited")
 (version 1 0)
 (library
  (part "776262-4"
   (description "Automotive Connectors 14 POS AMPSEAL VERTICAL HDR")
   (family "CON")
   (package "7762624")
   (attribute "Datasheet Link" "https://www.arrow.com/en/products/776262-4/te-connectivity")
   (attribute "Geometry.Height" "34.3mm")
   (attribute "Manufacturer_Name" "TE Connectivity")
   (attribute "Manufacturer_Part_Number" "776262-4")
   (attribute "Mouser Part Number" "571-776262-4")
   (attribute "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity/776262-4/?qs=tLAa1RwIH6cNE2syojWMEQ%3D%3D")
   (attribute "Arrow Part Number" "776262-4")
   (attribute "Arrow Price/Stock" "https://www.arrow.com/en/products/776262-4/te-connectivity")
   (gate
    (symbol "776262-4")
    (pin "1" 1 PS)
    (pin "2" 2 PS)
    (pin "3" 3 PS)
    (pin "4" 4 PS)
    (pin "5" 5 PS)
    (pin "6" 6 PS)
    (pin "7" 7 PS)
    (pin "8" 8 PS)
    (pin "9" 9 PS)
    (pin "10" 10 PS)
    (pin "11" 11 PS)
    (pin "12" 12 PS)
    (pin "13" 13 PS)
    (pin "14" 14 PS)
    (pin "MH1" MH1 PS)
    (pin "MH2" MH2 PS)
    (pin "MH3" MH3 PS)
    (pin "MH4" MH4 PS)
   )
  )
  (symbol "776262-4"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 200 100) (pt 700 100) (pt 700 -900) (pt 200 -900) (pt 200 100) (closed))
   )
   (terminal
    (body (symbol "PIN") (pt 0 0) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -100) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -200) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -300) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -400) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -500) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -600) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -700) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 -800) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 0) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -100) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -200) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -300) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -400) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -500) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -600) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -700) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 900 -800) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
  )
  (symbol "PIN"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 200 0))))
  (symbol "PINSHORT"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 100 0))))
  (package "7762624"
   (units MM)
   (layer TASM
    (graphic
     (stroke 0.2)
     (path
      (closed true)
      (pt -16.4 -20.05)
      (pt 32.4 -20.05)
      (pt 32.4 12.05)
      (pt -16.4 12.05)
      (pt -16.4 -20.05))))
   (layer TSLK
    (graphic
     (stroke 0.1)
     (path
      (closed true)
      (pt -16.4 12.05)
      (pt 32.4 12.05)
      (pt 32.4 -20.05)
      (pt -16.4 -20.05)
      (pt -16.4 12.05))))
   (layer OCCA
    (graphic
     (stroke 0.1)
     (path
      (closed true)
      (pt -17.4 13.05)
      (pt 33.4 13.05)
      (pt 33.4 -21.05)
      (pt -17.4 -21.05)
      (pt -17.4 13.05))))
   (leg 1 (pt 0.000 0.000) (padstack 1))
   (leg 2 (pt 4.000 0.000) (padstack 0))
   (leg 3 (pt 8.000 0.000) (padstack 0))
   (leg 4 (pt 12.000 0.000) (padstack 0))
   (leg 5 (pt 16.000 0.000) (padstack 0))
   (leg 6 (pt 2.000 -4.000) (padstack 0))
   (leg 7 (pt 6.000 -4.000) (padstack 0))
   (leg 8 (pt 10.000 -4.000) (padstack 0))
   (leg 9 (pt 14.000 -4.000) (padstack 0))
   (leg 10 (pt 0.000 -8.000) (padstack 0))
   (leg 11 (pt 4.000 -8.000) (padstack 0))
   (leg 12 (pt 8.000 -8.000) (padstack 0))
   (leg 13 (pt 12.000 -8.000) (padstack 0))
   (leg 14 (pt 16.000 -8.000) (padstack 0))
   (leg MH1 (pt -9.700 6.800) (padstack 15))
   (leg MH2 (pt 25.700 6.800) (padstack 16))
   (leg MH3 (pt -11.200 -11.300) (padstack 17))
   (leg MH4 (pt 27.200 -11.300) (padstack 18))
   (padstack 0
    (hole 1.85)
    (plated true)
    (pad (layer TCOP) (round 2.775))
    (pad (layer INNER) (round 2.775))
    (pad (layer BCOP) (round 2.775))
   )
   (padstack 1
    (hole 1.85)
    (plated true)
    (pad (layer TCOP) (square 2.775))
    (pad (layer INNER) (round 2.775))
    (pad (layer BCOP) (square 2.775))
   )
   (padstack 15
    (hole 2)
    (plated true)
    (pad (layer TCOP) (round 3.000))
    (pad (layer INNER) (round 3.000))
    (pad (layer BCOP) (round 3.000))
   )
   (padstack 16
    (hole 2)
    (plated true)
    (pad (layer TCOP) (round 3.000))
    (pad (layer INNER) (round 3.000))
    (pad (layer BCOP) (round 3.000))
   )
   (padstack 17
    (hole 2)
    (plated true)
    (pad (layer TCOP) (round 3.000))
    (pad (layer INNER) (round 3.000))
    (pad (layer BCOP) (round 3.000))
   )
   (padstack 18
    (hole 2)
    (plated true)
    (pad (layer TCOP) (round 3.000))
    (pad (layer INNER) (round 3.000))
    (pad (layer BCOP) (round 3.000))
   )
   (model "776262-4.stp"
    (euler 0 0 0)
    (offset 8 -4 34.290000915527344)
   )
  )
 )
)
