FILE_TYPE = MULTI_PHYS_TABLE;

PART 'IHLP2525CZER100M11'
CLASS = DISCRETE
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "ARROW_PART_NUMBER", "ARROW_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Vishay", "IHLP2525CZER100M11" (!) = "", "INDPM6965X300N", "Inductors Precision Moulded", "70-IHLP2525CZER100M1", "https://www.mouser.co.uk/ProductDetail/Vishay-Dale/IHLP2525CZER100M11?qs=gMuw6kkpPFi7WFZ9cEKRAA%3D%3D", "IHLP2525CZER100M11", "https://www.arrow.com/en/products/ihlp2525czer100m11/vishay?region=nac", "Vishay IHLP2525CZ-11 Series Shielded Wire-wound SMD Inductor with a Metal Composite Core, 10 uH +/-20% Wire-Wound 4A Idc", "https://componentsearchengine.com/Datasheets/2/IHLP2525CZER100M11.pdf", "3 mm"
END_PART

END.
