(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "LM5122MH_NOPB" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 31.75 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "LM5122MH_NOPB" (at 31.75 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SOP65P640X110-21N" (at 31.75 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://datasheet.datasheetarchive.com/originals/distributors/Datasheets-SFU2/DSASFU100037250.pdf" (at 31.75 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "65V Boost Controller with Phase HTSSOP20 LM5122MH/NOPB, DC-DC Controller, 15A, 65 V Step-Up, 250 kHz, 20-Pin, HTTSOP" (at 31.75 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1.1" (at 31.75 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Texas Instruments" (at 31.75 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "LM5122MH/NOPB" (at 31.75 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "595-LM5122MH/NOPB" (at 31.75 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM5122MH-NOPB?qs=iIeLWXrA%252B1WObMiZ4L5hVQ%3D%3D" (at 31.75 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "LM5122MH/NOPB" (at 31.75 -894.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/lm5122mhnopb/texas-instruments?region=nac" (at 31.75 -994.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 30.48 -30.48)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "SYNCOUT" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "OPT" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "CSN" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "CSP" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "VIN" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "UVLO" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "SS" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "SYNCIN/RT" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -20.32 0) (length 5.08)
      (name "AGND" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -22.86 0) (length 5.08)
      (name "FB" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 -35.56 90) (length 5.08)
      (name "EP" (effects (font (size 1.27 1.27))))
      (number "21" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 0 180) (length 5.08)
      (name "BST" (effects (font (size 1.27 1.27))))
      (number "20" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -2.54 180) (length 5.08)
      (name "HO" (effects (font (size 1.27 1.27))))
      (number "19" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -5.08 180) (length 5.08)
      (name "SW" (effects (font (size 1.27 1.27))))
      (number "18" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -7.62 180) (length 5.08)
      (name "VCC" (effects (font (size 1.27 1.27))))
      (number "17" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -10.16 180) (length 5.08)
      (name "LO" (effects (font (size 1.27 1.27))))
      (number "16" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -12.7 180) (length 5.08)
      (name "PGND" (effects (font (size 1.27 1.27))))
      (number "15" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -15.24 180) (length 5.08)
      (name "RES" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -17.78 180) (length 5.08)
      (name "MODE" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -20.32 180) (length 5.08)
      (name "SLOPE" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -22.86 180) (length 5.08)
      (name "COMP" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
  )
)
