(Japanese_coding: sjis)
(function "ECS_3637563"
    (uver 1)
    (cuser "SamacSys")
    (uuser "SamacSys")
    (ctime 2020-04-14-05:27:57)
    (utime 2023-10-03-04:07:38)
    (interface
        (port "1" (symbPinId 1) (portType INOUT))
        (port "2" (symbPinId 2) (portType INOUT))
    )
    (property "symbolName" "EEHZA1V271P")
)


(pinAssign "ECS_3637563"
    (uver 1)
    (cuser "SamacSys")
    (uuser "SamacSys")
    (ctime 2020-04-14-05:27:57)
    (utime 2023-10-03-04:07:38)
    (interface
        (port "1" (symbPinId 1) (portName "+") (portType INOUT))
        (port "2" (symbPinId 2) (portName "-") (portType INOUT))
    )
    (internal
        (funcInst (functionRef "ECS_3637563")
                (port "1" (match "1"))
                (port "2" (match "2"))
        )
    )
    (property "usePowerBox" "No")
    (property "symbolName" "EEHZA1V271P")
)


(part "EEHZA1V271P"
    (uver 1)
    (cuser "SamacSys")
    (uuser "SamacSys")
    (ctime 2020-04-14-05:27:57)
    (utime 2023-10-03-04:07:38)
    (packageRef "EEHZA1V271P")
    (pinAssignRef "ECS_3637563")
    (interface
        (port "1" (symbPinId 1) (portName "+") (portType INOUT))
        (port "2" (symbPinId 2) (portName "-") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "enetNonSeries" "NO")
    (property "refDesPrefix" "C")
    (property "description" "Cap Aluminum Polymer Hybrid 270uF 35VDC 20% (10 X 10.2mm) SMD 0.02 Ohm 2500mA 10000h 105C Automotive T/R")
    (property "Manufacturer_Name" "Panasonic")
    (property "Manufacturer_Part_Number" "EEHZA1V271P")
    (property "Mouser_Part_Number" "")
    (property "Mouser_Price/Stock" "")
    (property "Arrow_Part_Number" "")
    (property "Arrow_Price/Stock" "")
    (property "Datasheet_Link" "http://industrial.panasonic.com/cdbs/www-data/pdf/RDD0000/ABA0000C1221.pdf")
    (property "compAreaTopHeight" 10.5)
)


