(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "BAV199" (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 31.75 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "BAV199" (at 31.75 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SOT95P230X100-3N" (at 31.75 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV199.pdf" (at 31.75 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "BAV199 Nexperia Dual SMT Low Leakage Diode, Series, 85V 160mA, 3us, 3-Pin TO-236AB" (at 31.75 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1" (at 31.75 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Nexperia" (at 31.75 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "BAV199" (at 31.75 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "N/A" (at 31.75 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/BAV199?qs=vHuUswq2%252BsxAj%252B0n7XN4nQ%3D%3D" (at 31.75 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "" (at 31.75 -894.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "" (at 31.75 -994.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 30.48 -5.08)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "ANODE" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "CATHODE" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 0 180) (length 5.08)
      (name "COMMON" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
  )
)
