(footprint "AMPSEAL_35_Pin_Straight"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -10.422 0)
		(layer "F.SilkS")
		(uuid "a9815b8a-6178-4ae9-ab11-dd2f9cec26fa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "AMPSEAL_35_Pin_Straight"
		(at 0 -11.422 0)
		(layer "F.Fab")
		(uuid "37bb0fbf-01f7-4b2e-ba0e-6d4fcddf3c46")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6ceece1a-3fb8-4f2a-9bf7-a8dab88c4df3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2fac840e-cf05-4b1b-9161-600139db51c7")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2f28ea6c-e65d-477c-a0ed-08000dd98a40")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -38.45 -16.05)
		(end 38.45 -16.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Cmts.User")
		(uuid "36ce0513-2f4a-45e4-a665-cbea7101c4f9")
	)
	(fp_line
		(start -38.45 16.05)
		(end -38.45 -16.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Cmts.User")
		(uuid "fe7c60c0-b1a5-4d4d-8a99-2b70b2b514ec")
	)
	(fp_line
		(start -38.45 16.05)
		(end 38.45 16.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Cmts.User")
		(uuid "f60f8ea9-7caf-4e28-932f-3f2b0c5f6f71")
	)
	(fp_line
		(start 38.45 -16.05)
		(end 38.45 16.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Cmts.User")
		(uuid "ba314bd6-6ead-416c-bed9-2adfaf69367b")
	)
	(fp_circle
		(center -33.2 7.3)
		(end -30.2 7.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "e6cb7f64-6346-4b67-ae8f-b03dff9ed8c3")
	)
	(fp_circle
		(center -31.7 -10.8)
		(end -28.7 -10.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "9fe967a2-c617-4a82-8ae7-618d21510f41")
	)
	(fp_circle
		(center 31.7 -10.8)
		(end 34.7 -10.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "ae15a3da-3d97-48e8-9dc5-2448c3b0885f")
	)
	(fp_circle
		(center 33.2 7.3)
		(end 36.2 7.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "abbd654c-1394-4e40-9042-01567731713b")
	)
	(fp_text user "13"
		(at -25 0 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "0aa3a940-99e9-41a2-abcd-1ef3b315b542")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
			(justify mirror)
		)
	)
	(fp_text user "1"
		(at -26 -4 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "140242e2-01a6-4a85-9031-7f46857b78bb")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
			(justify mirror)
		)
	)
	(fp_text user "35"
		(at 27 4 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "8d4536b7-d60f-46aa-ab97-ae5b10478e29")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
			(justify mirror)
		)
	)
	(fp_text user "12"
		(at 27 -4 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "a13a0c92-1f21-421c-be27-4cc0c3cee2dc")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
			(justify mirror)
		)
	)
	(fp_text user "24"
		(at -27 4 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "a264f77f-de5f-42e9-95a6-a9c2f09f9b15")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
			(justify mirror)
		)
	)
	(fp_text user "23"
		(at 25 0 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "da60f6bf-dad2-4e5a-aa76-080d8fab1dcf")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
			(justify mirror)
		)
	)
	(fp_text user "23"
		(at 25 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "29916d3d-bdf2-418f-a476-ae6e275e706e")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
		)
	)
	(fp_text user "1"
		(at -26 -4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "72c99641-c2fd-44cd-986d-f8d46d9f474b")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
		)
	)
	(fp_text user "13"
		(at -25 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8cb816bc-7205-464f-9a45-681def19006e")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
		)
	)
	(fp_text user "24"
		(at -27 4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a7cd9869-5719-46bb-bf5b-04c5c7978a32")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
		)
	)
	(fp_text user "12"
		(at 27 -4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "eecfe77f-c4d8-42d3-a41b-ed5af312ec3e")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
		)
	)
	(fp_text user "35"
		(at 27.010361 3.967955 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "fefe6f81-2948-482b-b0e9-1214466df505")
		(effects
			(font
				(size 2 2)
				(thickness 0.3)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -33.2 7.3)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(uuid "1c34747a-88a0-4b9c-8872-8e801b5eeba8")
	)
	(pad "" np_thru_hole circle
		(at -31.7 -10.8)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(uuid "96dbb7d1-1525-4d71-82f4-8c34799547e0")
	)
	(pad "" np_thru_hole circle
		(at 31.7 -10.8)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(uuid "8d7b4de0-484d-4b22-bce8-900f396f7b3a")
	)
	(pad "" np_thru_hole circle
		(at 33.2 7.3)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(uuid "866af703-92cf-4f89-bf88-549d1db829d6")
	)
	(pad "1" thru_hole circle
		(at -22 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a3be8747-0c1b-4e5f-ada3-a8cb1445844d")
	)
	(pad "2" thru_hole circle
		(at -18 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7f320ab6-11f0-4c38-862a-91c74cd23679")
	)
	(pad "3" thru_hole circle
		(at -14 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "371bfdca-96a9-4765-9692-c64b2cf50c73")
	)
	(pad "4" thru_hole circle
		(at -10 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4d0ebafd-da45-44bc-ade9-70720135b445")
	)
	(pad "5" thru_hole circle
		(at -6 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e4af400a-23bf-438b-b582-785b3a7e5e31")
	)
	(pad "6" thru_hole circle
		(at -2 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "01c962f7-be30-468f-9d18-96e39311d3d4")
	)
	(pad "7" thru_hole circle
		(at 2 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2f87b7bb-afad-4203-ab8b-fa3475cc0b3a")
	)
	(pad "8" thru_hole circle
		(at 6 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c6d00b66-52eb-41f7-98ef-7bb5270766f0")
	)
	(pad "9" thru_hole circle
		(at 10 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fb1c6806-02f3-4ade-abf7-6979b4c3cdd1")
	)
	(pad "10" thru_hole circle
		(at 14 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "790193b6-4659-4e1e-95ff-da7be6a9b676")
	)
	(pad "11" thru_hole circle
		(at 18 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "64404a68-c4d4-4107-8ff3-d6694b9eab76")
	)
	(pad "12" thru_hole circle
		(at 22 -4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b5f07e5a-3a27-4874-9256-95b07294a0ba")
	)
	(pad "13" thru_hole circle
		(at -20 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "485a0d42-412f-4930-af39-4a2ebecbca6a")
	)
	(pad "14" thru_hole circle
		(at -16 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "58df3a68-88e3-4629-b2c4-6de82d0b214b")
	)
	(pad "15" thru_hole circle
		(at -12 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "00aeff10-0d83-4450-8960-340884f1cfb9")
	)
	(pad "16" thru_hole circle
		(at -8 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2d2ab1e9-30f7-420d-8d24-257e66b02900")
	)
	(pad "17" thru_hole circle
		(at -4 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "acc2d76a-9046-4f52-880f-939e232e0036")
	)
	(pad "18" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "483e3f1f-05d1-4fd6-be86-9699ce9276ad")
	)
	(pad "19" thru_hole circle
		(at 4 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "53890c45-2762-4c04-9be5-25e313bd1535")
	)
	(pad "20" thru_hole circle
		(at 8 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "670fe258-8d3b-4620-853a-7ce87a6fa1be")
	)
	(pad "21" thru_hole circle
		(at 12 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9fe712a4-c37b-4951-abf2-12b05d61ed35")
	)
	(pad "22" thru_hole circle
		(at 16 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4c5653f3-6d87-42b0-a076-716989e787c5")
	)
	(pad "23" thru_hole circle
		(at 20 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a6b050d5-3b2a-43e9-ac1d-6e71d067b308")
	)
	(pad "24" thru_hole circle
		(at -22 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cb6a4e67-4c01-4eac-9688-56e49e5f3fef")
	)
	(pad "25" thru_hole circle
		(at -18 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "91d04dcb-34c5-4924-bc63-29c1d3313333")
	)
	(pad "26" thru_hole circle
		(at -14 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9976e781-8e7a-420f-9b15-5f6b7068c2bb")
	)
	(pad "27" thru_hole circle
		(at -10 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "219c2c93-5504-4d3c-b7a4-2bc491f8947c")
	)
	(pad "28" thru_hole circle
		(at -6 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "243f298e-2793-44b3-9d54-4712a1ecb730")
	)
	(pad "29" thru_hole circle
		(at -2 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e080ac50-6532-4739-8d0b-2a4f22a2bff7")
	)
	(pad "30" thru_hole circle
		(at 2 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dc42fccf-7724-4a1b-b707-1a51314aabe6")
	)
	(pad "31" thru_hole circle
		(at 6 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "75fd6d1e-4891-446e-8c47-765aadf477de")
	)
	(pad "32" thru_hole circle
		(at 10 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7fe521bc-8da4-418f-b1a1-31449f25f879")
	)
	(pad "33" thru_hole circle
		(at 14 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ec5214a2-6b9d-46d5-86da-7c67e41bd23b")
	)
	(pad "34" thru_hole circle
		(at 18 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "647e504a-ee3f-479c-836a-27d895e5e44e")
	)
	(pad "35" thru_hole circle
		(at 22 4)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "68fcb171-13e7-4d35-9516-7eb06a5236ae")
	)
	(model "${KIPRJMOD}/libraries/c-1-776231-4-d-3d.stp"
		(offset
			(xyz 0 0 34.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)