(part "BAV199"
    (packageRef "SOT95P230X100-3N")
    (interface
        (port "1" (symbPinId 1) (portName "ANODE") (portType INOUT))
        (port "2" (symbPinId 2) (portName "CATHODE") (portType INOUT))
        (port "3" (symbPinId 3) (portName "COMMON") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "compKind" "122")
    (property "Manufacturer_Name" "Nexperia")
    (property "Manufacturer_Part_Number" "BAV199")
    (property "Mouser_Part_Number" "N/A")
    (property "Mouser_Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/BAV199?qs=vHuUswq2%252BsxAj%252B0n7XN4nQ%3D%3D")
    (property "Arrow_Part_Number" "")
    (property "Arrow_Price/Stock" "")
    (property "Description" "BAV199 Nexperia Dual SMT Low Leakage Diode, Series, 85V 160mA, 3us, 3-Pin TO-236AB")
    (property "Datasheet_Link" "https://assets.nexperia.com/documents/data-sheet/BAV199.pdf")
    (property "symbolName1" "BAV199")
)
