(footprint "AMPSEAL_23_Pin_Straight" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -10.922) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4d2a5be0-a08d-4c6c-82bd-0d89093f9d70)
  )
  (fp_text value "AMPSEAL_23_Pin_Straight" (at 0 -12.692) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 316740e7-8088-4086-b953-79d08c2040da)
  )
  (fp_text user "15" (at 17 0 unlocked) (layer "B.SilkS")
      (effects (font (size 2 2) (thickness 0.3)) (justify mirror))
    (tstamp 1408448d-2ea4-4897-8af6-330cc932dfe0)
  )
  (fp_text user "9" (at -16 0 unlocked) (layer "B.SilkS")
      (effects (font (size 2 2) (thickness 0.3)) (justify mirror))
    (tstamp 7163ffa9-420f-4be8-b531-778124f843b5)
  )
  (fp_text user "23" (at 19 4 unlocked) (layer "B.SilkS")
      (effects (font (size 2 2) (thickness 0.3)) (justify mirror))
    (tstamp 74f8bc29-00fa-442d-a357-387b6b0ebe4b)
  )
  (fp_text user "8" (at 18 -4 unlocked) (layer "B.SilkS")
      (effects (font (size 2 2) (thickness 0.3)) (justify mirror))
    (tstamp 8b3b794b-d920-4f90-a2c0-241eab321905)
  )
  (fp_text user "1" (at -18 -4 unlocked) (layer "B.SilkS")
      (effects (font (size 2 2) (thickness 0.3)) (justify mirror))
    (tstamp a180564c-2664-42b0-adb2-a03be1b21949)
  )
  (fp_text user "16" (at -19 4 unlocked) (layer "B.SilkS")
      (effects (font (size 2 2) (thickness 0.3)) (justify mirror))
    (tstamp d2aaec98-1d1e-471b-a34d-ed6d7271873e)
  )
  (fp_text user "1" (at -18 -4 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.3)))
    (tstamp 31a167a4-211d-4f8d-ad54-7d4808aaf848)
  )
  (fp_text user "16" (at -19 4 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.3)))
    (tstamp 7f501651-7a88-47eb-a23c-4632e47a43ae)
  )
  (fp_text user "9" (at -16 0 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.3)))
    (tstamp 853e86e2-a453-4f1c-9a56-bb2f3b0c1146)
  )
  (fp_text user "23" (at 19 4 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.3)))
    (tstamp c5ba6f9d-5a35-4228-b998-435631b79f30)
  )
  (fp_text user "8" (at 18 -4 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.3)))
    (tstamp c5c76dcf-ef78-4d2e-89be-7c85577aa6bc)
  )
  (fp_text user "15" (at 17 0 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.3)))
    (tstamp e5cd4778-0df8-4f28-a565-0b6e05aab5c5)
  )
  (fp_line (start -30.4 -16.05) (end 30.4 -16.05)
    (stroke (width 0.12) (type solid)) (layer "Cmts.User") (tstamp 7ae0021e-54de-4a62-bc76-11533b7b66b2))
  (fp_line (start -30.4 16.05) (end -30.4 -16.05)
    (stroke (width 0.12) (type solid)) (layer "Cmts.User") (tstamp a3cb7cfb-722a-4db7-a5ef-00d323e65dee))
  (fp_line (start -30.4 16.05) (end 30.4 16.05)
    (stroke (width 0.12) (type solid)) (layer "Cmts.User") (tstamp 6be9d1b8-ded6-4858-b568-a9ccddfd00e3))
  (fp_line (start 30.4 -16.05) (end 30.4 16.05)
    (stroke (width 0.12) (type solid)) (layer "Cmts.User") (tstamp 7f3a48e3-70ab-48c6-a79c-ad3a7f7e6f2a))
  (fp_circle (center -25.2 7.3) (end -22.2 7.3)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 27398652-e43c-4df8-803b-6b183928c941))
  (fp_circle (center -23.7 -10.8) (end -20.7 -10.8)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f935fdbe-0eea-4a38-87ef-ec4ca1c1a071))
  (fp_circle (center 23.7 -10.8) (end 26.7 -10.8)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 989cdf69-94dc-4f95-a6b2-379f55481695))
  (fp_circle (center 25.2 7.3) (end 28.2 7.3)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 7ce4f852-b716-40be-ac7d-7cb143001b4b))
  (pad "" np_thru_hole circle (at -25.2 7.3) (size 2 2) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 9acfd92d-6040-40b4-8240-8e61ca0b42d2))
  (pad "" np_thru_hole circle (at -23.7 -10.8) (size 2 2) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 3a06a601-9966-4715-af66-6028ce40155c))
  (pad "" np_thru_hole circle (at 23.7 -10.8) (size 2 2) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 66b0d3fa-ad56-43a2-a595-755138983138))
  (pad "" np_thru_hole circle (at 25.2 7.3) (size 2 2) (drill 2) (layers "*.Cu" "*.Mask") (tstamp fff4ef46-fa7e-427d-8101-71d0e9a20af2))
  (pad "1" thru_hole circle (at -14 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 688390f9-e3e1-40b7-8bd5-c0df106f8032))
  (pad "2" thru_hole circle (at -10 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 44df55da-2ed5-47d6-be26-b3e8546cf795))
  (pad "3" thru_hole circle (at -6 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp bb1c2776-eb68-4020-9b3c-daf0b4aab4ce))
  (pad "4" thru_hole circle (at -2 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 91527fb0-67eb-4cf1-b6b9-3d6608f77576))
  (pad "5" thru_hole circle (at 2 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp abc034df-7288-4dce-b60d-ed40f4349d8d))
  (pad "6" thru_hole circle (at 6 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp aa5a4b16-1c94-4475-9121-8ec5ebb95bab))
  (pad "7" thru_hole circle (at 10 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp e57cede2-ed5a-4d54-9b98-31040c6c47d2))
  (pad "8" thru_hole circle (at 14 -4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp e95326be-0cae-4c88-9120-d7af0822bd9d))
  (pad "9" thru_hole circle (at -12 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 8c6d4763-05bf-4ee2-99b0-f30fbff0a7cf))
  (pad "10" thru_hole circle (at -8 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp d7920ed5-dabc-44ee-be1b-aeec3eef16fc))
  (pad "11" thru_hole circle (at -4 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp cb09b810-d65c-47cd-af20-a009724d52e0))
  (pad "12" thru_hole circle (at 0 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp d8c5b5b8-2bd9-43ea-a6be-667ba4a7f77f))
  (pad "13" thru_hole circle (at 4 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 930e7adb-a564-4805-9ea5-f3a5f2d15d6a))
  (pad "14" thru_hole circle (at 8 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp ed959c6b-51e6-4a0a-837c-d654cda10a6a))
  (pad "15" thru_hole circle (at 12 0) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp cc971b16-8a78-45c8-9461-fd0ffe3d6fb8))
  (pad "16" thru_hole circle (at -14 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 9c51ae1a-a739-4e95-94a0-e1ffd900507d))
  (pad "17" thru_hole circle (at -10 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 811d24d5-2c39-4cc3-b1ef-08fa4acb0bda))
  (pad "18" thru_hole circle (at -6 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp b0a16f27-a9b1-4274-86b4-27fed5e75621))
  (pad "19" thru_hole circle (at -2 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 4fcd2dcd-da35-42ad-b8ed-55c7c013a552))
  (pad "20" thru_hole circle (at 2 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp c8ea8353-2ae1-48f8-869e-23c36f898724))
  (pad "21" thru_hole circle (at 6 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 6811dd58-375c-4d80-a70c-fc6f46a352c4))
  (pad "22" thru_hole circle (at 10 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp f7776023-14ec-42c9-becf-3daf06aea040))
  (pad "23" thru_hole circle (at 14 4) (size 3 3) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 81322c0d-c6c2-4a69-9068-ddaec12458b7))
  (model "${KIPRJMOD}/3d_Models/c-1-776228-4-e-3d.stp"
    (offset (xyz 0 0 34))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
