(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "BTS7004-1EPP" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BTS7004-1EPP" (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:Infineon_PG-TSDSO-14-22" (at -25.4 -16.51 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS7004-1EPP-DS-v01_00-EN.pdf?fileId=5546d4626102d35a016147550a725555" (at -1.27 -19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BTS7004" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Smart High-Side Power Switch, PROFET, One Channel, 12V, 15A, Rds(on) 4.4mΩ, PG-TSDSO-14-22" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*TSDSO*22*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BTS7004-1EPP_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "BTS7004-1EPP_1_1"
      (pin power_in line (at -7.62 2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -8.89 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -6.35 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -3.81 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -1.27 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 1.27 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -1.27 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -3.81 0) (length 2.54)
        (name "DEN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 -6.35 0) (length 2.54)
        (name "IS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -8.89 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -11.43 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -13.97 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -13.97 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -11.43 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BTS7002-1EPP" (extends "BTS7004-1EPP")
    (property "Reference" "U" (at -3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BTS7002-1EPP" (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -22.86 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BTS7004" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Smart High-Side Power Switch, PROFET, One Channel, 12V, 21A, Rds(on) 2.6mΩ, PG-TSDSO-14-22" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*TSDSO*22*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "BTS7008-1EPZ" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BTS7008-1EPZ" (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:Infineon_PG-TSDSO-14-22" (at -25.4 -16.51 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS7004-1EPP-DS-v01_00-EN.pdf?fileId=5546d4626102d35a016147550a725555" (at -1.27 -19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BTS7004" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Smart High-Side Power Switch, PROFET, One Channel, 12V, 15A, Rds(on) 4.4mΩ, PG-TSDSO-14-22" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*TSDSO*22*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BTS7008-1EPZ_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "BTS7008-1EPZ_1_1"
      (pin power_in line (at -7.62 2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -8.89 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -6.35 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -3.81 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -1.27 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 1.27 180) (length 2.54)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -1.27 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -3.81 0) (length 2.54)
        (name "DEN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 -6.35 0) (length 2.54)
        (name "IS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -8.89 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -11.43 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -13.97 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -13.97 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -11.43 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BTS7020-2EPA(M)" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BTS7020-2EPA(M)" (at 6.35 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:Infineon_PG-TSDSO-14-22" (at -22.86 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS7004-1EPP-DS-v01_00-EN.pdf?fileId=5546d4626102d35a016147550a725555" (at -1.27 -7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BTS7004" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Smart High-Side Power Switch, PROFET, Two Channel, 12V, 5A, Rds(on) 23.7mΩ, PG-TSDSO-14-22" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*TSDSO*22*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BTS7020-2EPA(M)_0_0"
      (pin input line (at -8.89 -1.27 0) (length 2.54)
        (name "DSEL" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 5.08 0) (length 2.54)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "BTS7020-2EPA(M)_0_1"
      (rectangle (start -6.35 10.16) (end 6.35 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "BTS7020-2EPA(M)_1_1"
      (pin power_in line (at 0 -11.43 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 8.89 6.35 180) (length 2.54) hide
        (name "OUT0" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 8.89 8.89 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 8.89 -7.62 180) (length 2.54)
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 8.89 -5.08 180) (length 2.54) hide
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 8.89 -10.16 180) (length 2.54) hide
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 7.62 0) (length 2.54)
        (name "IN0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 1.27 0) (length 2.54)
        (name "DEN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -8.89 -3.81 0) (length 2.54)
        (name "IS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 8.89 8.89 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 8.89 3.81 180) (length 2.54)
        (name "OUT0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 8.89 1.27 180) (length 2.54) hide
        (name "OUT0" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BTS7120-2EPA" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BTS7120-2EPA" (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:Infineon_PG-TSDSO-14-22" (at -22.86 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS7120-2EPA-DataSheet-v01_10-EN.pdf?fileId=5546d462636cc8fb016421dc08d31138" (at -3.81 -19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BTS7004" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Smart High-Side Power Switch, PROFET, Two Channel, 12V, 5A, Rds(on) 23.7mΩ, PG-TSDSO-14-22" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*TSDSO*22*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BTS7120-2EPA_0_0"
      (pin input line (at -8.89 -2.54 0) (length 2.54)
        (name "DSEL" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 2.54 0) (length 2.54)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "BTS7120-2EPA_0_1"
      (rectangle (start -6.35 10.16) (end 6.35 -11.43)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "BTS7120-2EPA_1_1"
      (pin power_out line (at -8.89 7.62 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 -5.08 180) (length 2.54)
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 8.89 -1.27 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 2.54 180) (length 2.54)
        (name "OUT0" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 5.08 180) (length 2.54)
        (name "OUT0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 7.62 180) (length 2.54)
        (name "OUT0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 5.08 0) (length 2.54)
        (name "IN0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 0 0) (length 2.54)
        (name "DEN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -8.89 -7.62 0) (length 2.54)
        (name "IS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -8.89 -10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 -10.16 180) (length 2.54)
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 -7.62 180) (length 2.54)
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BTS7020-2EPA" (extends "BTS7120-2EPA")
    (property "Reference" "U" (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BTS7020-2EPA" (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -22.86 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -3.81 -19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BTS7004" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Smart High-Side Power Switch, PROFET, Two Channel, 12V, 5A, Rds(on) 23.7mΩ, PG-TSDSO-14-22" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*TSDSO*22*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
)
