(footprint "Finder_RBR"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "cffa72c6-6669-4138-b3b7-a00513894016")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Finder_RBR"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9bfd6c49-7444-41ef-9674-4b14cca4bfb4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d40bfe70-e02f-4487-b96b-904d9a53bc1d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5f0da7c3-bd57-4670-b968-7d0d9a5f68c8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8dcca390-be9b-4254-b445-1ae61b352ace")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -5.325 4.375)
		(end 23.675 16.775)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "81a90369-d7dd-459a-bea8-103fdff32e1b")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4c76f472-347d-41b0-8343-1f504e58f4d0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "11" thru_hole circle
		(at 17.725 6.75)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8421d1ca-a0c0-4386-a46f-290bd602c592")
	)
	(pad "12" thru_hole circle
		(at 12.725 6.75)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "06f30ba3-ecb3-438c-957a-433ac0a7bf5b")
	)
	(pad "14" thru_hole circle
		(at 22.725 6.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eb963ee6-5140-4cf7-97ef-a8d9fcdecac4")
	)
	(pad "21" thru_hole circle
		(at 17.7 14.25)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "22625b91-723b-41d6-9037-c72ecea95ddc")
	)
	(pad "22" thru_hole circle
		(at 12.7 14.25)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bbc36ca6-d42a-4a7b-b107-667a06c917e0")
	)
	(pad "24" thru_hole circle
		(at 22.7 14.3)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "03709282-8109-4c35-bba2-0f262a6bda32")
	)
	(pad "A1" thru_hole circle
		(at -2.8 6.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4c71cb89-55a9-4a6c-af3e-0e9b6d48b8d5")
	)
	(pad "A2" thru_hole circle
		(at -2.825 14.3)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a26c411d-7652-4f23-affd-0145105d6fd9")
	)
)
