(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "BTS3405G" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 36.83 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "BTS3405G" (at 36.83 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SOIC127P600X175-8N" (at 36.83 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS3405G-DS-v01_01-en.pdf?fileId=db3a30431689f4420116d43d769b0cc0" (at 36.83 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Infineon BTS3405G Digital Power Switch IC, Smart Low-Side, 350mA, 10V, 8-Pin, SO" (at 36.83 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1.75" (at 36.83 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Infineon" (at 36.83 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "BTS3405G" (at 36.83 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "" (at 36.83 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "" (at 36.83 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 35.56 -10.16)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "SOURCE_1" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "IN1" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "SOURCE_2" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "IN2" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 0 180) (length 5.08)
      (name "DRAIN_1_2" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -2.54 180) (length 5.08)
      (name "DRAIN_1_1" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -5.08 180) (length 5.08)
      (name "DRAIN_2_2" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -7.62 180) (length 5.08)
      (name "DRAIN_2_1" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
  )
)
