<?xml version="1.0" encoding="utf-8"?>
<!--/943922/1272411/2.50/3/4/Diode/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;BAV199 Nexperia Dual SMT Low Leakage Diode, Series, 85V 160mA, 3us, 3-Pin TO-236AB&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P230X100-3N">
<description>&lt;b&gt;SOT-23&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="BAV199">
<pin name="ANODE" direction="io"/>
<pin name="CATHODE" direction="io"/>
<pin name="COMMON" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BAV199" prefix="D">
<description>&lt;b&gt;BAV199 Nexperia Dual SMT Low Leakage Diode, Series, 85V 160mA, 3us, 3-Pin TO-236AB&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://assets.nexperia.com/documents/data-sheet/BAV199.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="BAV199"/>
</gates>
<devices>
<device name="" package="SOT95P230X100-3N">
<connects>
<connect gate="G$1" pin="ANODE" pad="1"/>
<connect gate="G$1" pin="CATHODE" pad="2"/>
<connect gate="G$1" pin="COMMON" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="Manufacturer_Name" value="Nexperia"/>
<attribute name="Manufacturer_Part_Number" value="BAV199"/>
<attribute name="Mouser_Part_Number" value="N/A"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Nexperia/BAV199?qs=vHuUswq2%252BsxAj%252B0n7XN4nQ%3D%3D"/>
<attribute name="Arrow_Part_Number" value=""/>
<attribute name="Arrow_Price-Stock" value=""/>
<attribute name="Description" value="BAV199 Nexperia Dual SMT Low Leakage Diode, Series, 85V 160mA, 3us, 3-Pin TO-236AB"/>
<attribute name="Height" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
