(footprint "Molex_iGrid_2x06"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole angled pin header, 2x08, 2.00mm pitch, 4.2mm pin length, double rows")
	(tags "Through hole angled pin header THT 2x08 2.00mm double row")
	(property "Reference" "J3"
		(at 0 -2 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "17dd9677-fbe9-4308-bb8c-a1b4b2e57c16")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "S_R"
		(at 4.1 13 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8c7a8829-ef82-4f63-9d9e-2eb140397117")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_2x08_P2.00mm_Horizontal"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f001444f-3cea-4cac-b792-6dac76ccf81e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "07817986-29ad-4ae5-85ae-8f3063a49193")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6bf03395-9bc1-4e1f-a709-b1f4e7f501b9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.5 -0.5)
		(end -2.5 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a7e4cd11-d65c-4724-9806-b3d9ce2d98ec")
	)
	(fp_line
		(start -2.5 12)
		(end -2.5 10.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "52f8b0a3-4b1b-49cb-bafd-e71ac604ebcd")
	)
	(fp_line
		(start -2 -0.5)
		(end -2.5 -0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "98d3f46e-a74e-4489-a826-eb2769454e36")
	)
	(fp_line
		(start -2 0.5)
		(end -1.5 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c7d2b908-e492-454d-9974-e05b94eb755d")
	)
	(fp_line
		(start -2 1.5)
		(end -2 0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "999bbc0d-0c57-4496-a1f1-317857c48df4")
	)
	(fp_line
		(start -2 2.5)
		(end -1.5 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "83068107-41ae-4ea2-8ccc-b14d371d21f9")
	)
	(fp_line
		(start -2 3.5)
		(end -2 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0f6ae844-6b07-472b-b913-fddd00a7cd8a")
	)
	(fp_line
		(start -2 4.5)
		(end -1.5 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2454ab28-0f69-4b2e-8013-3c0ae2c53e6a")
	)
	(fp_line
		(start -2 5.5)
		(end -2 4.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f06dc7d9-6178-4912-8a78-ca9910774dd9")
	)
	(fp_line
		(start -2 6.5)
		(end -1.5 6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c2c4bdd3-6a54-46a7-afaf-f80a0b385cae")
	)
	(fp_line
		(start -2 7.5)
		(end -2 6.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "52197c6e-e437-4137-8541-ec0d70cedf90")
	)
	(fp_line
		(start -2 8.5)
		(end -1.5 8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6a80178e-e499-4439-a6c8-2361a3da96ea")
	)
	(fp_line
		(start -2 9.5)
		(end -2 8.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "83f5b706-aded-43da-b6fc-441b52d482e3")
	)
	(fp_line
		(start -2 10.5)
		(end -2.5 10.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4de0759f-c415-407c-a702-2d4a291c2a45")
	)
	(fp_line
		(start -2 10.5)
		(end -1.5 10)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "01afcb54-458a-4763-b7aa-4cf4bce9687d")
	)
	(fp_line
		(start -1.5 0)
		(end -2 -0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b07985fb-9d21-4c7c-bd8c-4cca19911256")
	)
	(fp_line
		(start -1.5 2)
		(end -2 1.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "29ac6989-dd2d-40dc-931c-bd468c9b628d")
	)
	(fp_line
		(start -1.5 4)
		(end -2 3.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8f7d6675-5d30-49bd-bed3-5a5a244f76ba")
	)
	(fp_line
		(start -1.5 6)
		(end -2 5.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2d75c295-f798-44ac-9cb6-95c91f3767b8")
	)
	(fp_line
		(start -1.5 8)
		(end -2 7.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "47abb454-ebbd-4d00-8471-3ddd649d2094")
	)
	(fp_line
		(start -1.5 10)
		(end -2 9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b26b780c-5258-4a7d-9334-794d64850809")
	)
	(fp_line
		(start 10 -2)
		(end -2.5 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e027831c-8bad-415e-86d7-fa4752debd71")
	)
	(fp_line
		(start 10 12)
		(end -2.5 12)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2597d8dd-896d-47a5-95a0-8b022f16a05e")
	)
	(fp_line
		(start 10 12)
		(end 10 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "37dc629d-7554-4862-bd14-75b9b28df972")
	)
	(fp_rect
		(start -2.5 -2)
		(end 10 12)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "097600b9-4ca5-4a03-8db2-4934e218697a")
	)
	(pad "1" thru_hole circle
		(at 1 0)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a2803414-831f-4a83-b1e6-56dfcfbf02b6")
	)
	(pad "2" thru_hole oval
		(at -1 0)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7664d141-cbc4-4d1c-b5b3-0a1f200e126e")
	)
	(pad "3" thru_hole oval
		(at 1 2)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2eb08d7c-44bd-442b-ae03-2e758364a3af")
	)
	(pad "4" thru_hole oval
		(at -1 2)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9aa24422-c92c-432b-b0e2-6a34245d0db4")
	)
	(pad "5" thru_hole oval
		(at 1 4)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4ac51cf3-fac3-4e57-a997-e1f581b6da05")
	)
	(pad "6" thru_hole oval
		(at -1 4)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d115a2eb-b62f-4d16-86b2-76754b2ab91c")
	)
	(pad "7" thru_hole oval
		(at 1 6)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2fa632c3-d9b0-4bab-8231-18b551193b46")
	)
	(pad "8" thru_hole oval
		(at -1 6)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6fde9942-5c72-41a2-b171-3289cb3fcf05")
	)
	(pad "9" thru_hole oval
		(at 1 8)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e1f150d4-6706-41a6-8654-d3a6362a1f4f")
	)
	(pad "10" thru_hole oval
		(at -1 8)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8cdb814d-3aac-4d59-b0ed-8e78a8a0583e")
	)
	(pad "11" thru_hole oval
		(at 1 10)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0856f084-16a1-45c8-a166-3e5a97aab509")
	)
	(pad "12" thru_hole oval
		(at -1 10)
		(size 1.35 1.35)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e6b870dd-022c-4bb9-be64-13be6194032f")
	)
	(model "${KIPRJMOD}/library/2086591240.stp"
		(offset
			(xyz 13 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
