(footprint "MagI3C-FDSM-SIP-3"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "173010342")
	(tags "Power Supply,  SIP-3, FDSM ")
	(property "Reference" "U**"
		(at 2.1668 2.25 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "805d35dd-a37f-489b-88b8-93d81c1297c4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(property "Value" "MagI3C-FDSM-SIP-3"
		(at 2.1668 2.25 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "0546fe5a-8f22-4308-914e-f30e520ae8f2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(property "Footprint" "Package_SIP:SIP3_11.6x8.5mm"
		(at 0.0468 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e75f8d92-9195-4edd-8a6c-ce12466f3043")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.we-online.com/components/products/datasheet/173010342.pdf"
		(at 0.0468 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c7cd8ad3-9cc4-408b-9819-b719bc92fdcf")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "The FDSM series of the MagI3C Power Module family is a fixed output voltage, fully integrated dc/dc power supply. The module integrates the switching power stage, control circuitry, inductor and capacitors all in one package."
		(at 0.0468 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f78f8157-26a8-48f7-bc0e-5e715c88ed56")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5.9 -4.118)
		(end 5.9 -4.118)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "01c3b558-d644-4917-a8a3-ecfd9397d287")
	)
	(fp_line
		(start -5.9 2.582)
		(end -5.9 -4.118)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5a1e1a68-e0cb-43d2-810d-a52628ad4687")
	)
	(fp_line
		(start -4 4.582)
		(end 5.9 4.582)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a888b3b0-bdc6-425a-b946-4270775878f8")
	)
	(fp_line
		(start 5.9 -4.118)
		(end 5.9 4.582)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "71be3c83-ec9e-40c7-831b-e2ff96d71c68")
	)
	(fp_line
		(start -6.1 4.782)
		(end -6.1 -4.318)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "aa3e7025-27f4-4c47-b998-0331155cf5f5")
	)
	(fp_line
		(start 6.1 -4.318)
		(end -6.1 -4.318)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "24bdc3ce-6fef-45c8-8da8-b0004e1a18bb")
	)
	(fp_line
		(start 6.1 4.782)
		(end -6.1 4.782)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c2a9e752-6804-49de-8484-e6f736f3bb73")
	)
	(fp_line
		(start 6.1 4.782)
		(end 6.1 -4.318)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "63cfb2ec-69e5-4764-9ee8-f66423bb2b63")
	)
	(fp_line
		(start -5.8 -4.018)
		(end -5.8 2.982)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cdf73193-782f-40ad-9811-9cba4ff700bd")
	)
	(fp_line
		(start -5.8 2.982)
		(end -4.3 4.482)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a7b8dd89-3e28-4b5f-a0ec-1bcaad0409b1")
	)
	(fp_line
		(start 5.8 -4.018)
		(end -5.8 -4.018)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "011dd2e8-046a-4f61-a619-0513b69fc85a")
	)
	(fp_line
		(start 5.8 4.482)
		(end -4.3 4.482)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1bc7349c-f5fe-43f7-b9d1-73013e70cc13")
	)
	(fp_line
		(start 5.8 4.482)
		(end 5.8 -4.018)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ec7ae3f7-dbfa-4f2f-a7d4-0fc791d53f99")
	)
	(fp_text user "${REFERENCE}"
		(at 2.1668 2.25 0)
		(layer "F.Fab")
		(uuid "051e7197-f89f-48fa-815a-04da9142cbc0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.218 180)
		(layer "F.Fab")
		(uuid "5acda6a5-bd9c-40ad-855c-1ad9c444fc0f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -2.54 2.482 270)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f1ecc875-c41f-4ec0-9096-29af511d0a5e")
	)
	(pad "2" thru_hole circle
		(at 0 2.482 180)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f688b9d2-7922-4e99-9d4c-6b8a36b76cc0")
	)
	(pad "3" thru_hole circle
		(at 2.54 2.482 270)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "36c8bf38-5406-4865-873c-cf27424e93fc")
	)
	(model "${KIPRJMOD}/KiCAD_Libraries/FaSTTUBe_Voltage_Regulators.pretty/3d_models/173010342.stp"
		(offset
			(xyz 0 -0.25 5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
