(footprint "JLC_PCBA_ToolingHole_1.152mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "e6974f77-0de6-4cc5-82b5-c4ec04d22bca")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "JLC_PCBA_ToolingHole_1.152mm"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "3a586f74-4ca8-4a9b-8aaf-99287def24eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3f2fce66-1dec-4993-961e-0661555ca6f0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fa72b5f4-445c-40de-8e6a-dd38d01c24a7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f61922b-62fc-4dd8-985f-993c5608808d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole board_only exclude_from_bom allow_missing_courtyard)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9c7bbb75-1acb-43b5-9e4b-38cad726843b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 1.3 1.3)
		(drill 1.152)
		(layers "F&B.Cu" "*.Mask")
		(clearance 0.124)
		(uuid "c8299bab-c124-4148-957d-e3b5c82cddfa")
	)
)
