(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "0603_green" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (id 0) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "0603_green" (id 1) (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 0 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "LED diode green" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LED green 150060VS75000" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "0603_green_0_1"
      (polyline
        (pts
          (xy -1.27 -1.27)
          (xy -1.27 1.27)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 0)
          (xy 1.27 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -1.27)
          (xy 1.27 1.27)
          (xy -1.27 0)
          (xy 1.27 -1.27)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.048 -0.762)
          (xy -4.572 -2.286)
          (xy -3.81 -2.286)
          (xy -4.572 -2.286)
          (xy -4.572 -1.524)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.778 -0.762)
          (xy -3.302 -2.286)
          (xy -2.54 -2.286)
          (xy -3.302 -2.286)
          (xy -3.302 -1.524)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "0603_green_1_1"
      (pin passive line (at -3.81 0 0) (length 2.54)
        (name "K" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.81 0 180) (length 2.54)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "0603_red" (extends "0603_green")
    (property "Reference" "D" (id 0) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "0603_red" (id 1) (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 0 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "LED diode red" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LED red 150060RS75000" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "CLQ6A_RGB(W)" (in_bom yes) (on_board yes)
    (property "Reference" "D?" (id 0) (at 0 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "CLQ6A_RGB(W)" (id 1) (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CLQ6A_RGB(W)_0_1"
      (rectangle (start -5.08 6.35) (end 5.08 -6.35)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "CLQ6A_RGB(W)_1_1"
      (pin power_in line (at -7.62 3.81 0) (length 2.54)
        (name "R+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 1.27 0) (length 2.54)
        (name "G+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 -1.27 0) (length 2.54)
        (name "B+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 -3.81 0) (length 2.54)
        (name "W+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -3.81 180) (length 2.54)
        (name "W-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -1.27 180) (length 2.54)
        (name "B-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 1.27 180) (length 2.54)
        (name "G-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 3.81 180) (length 2.54)
        (name "R-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Dual_Blue{slash}Yellow" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (id 0) (at 0 5.715 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Dual_Blue{slash}Yellow" (id 1) (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "LED_SMD:LED_RGB_Wuerth-PLCC4_3.2x2.8mm_150141M173100" (id 2) (at 0 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 0.762 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "LED diode bicolor dual" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Bicolor LED, blue and yellow, 150141YB73100" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Dual_Blue{slash}Yellow_0_1"
      (polyline
        (pts
          (xy -5.08 -2.54)
          (xy 2.032 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54)
          (xy 2.032 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -1.27)
          (xy 1.27 -3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 3.81)
          (xy 1.27 1.27)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -2.54)
          (xy 1.905 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 1.905 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -1.27)
          (xy -1.27 -3.81)
          (xy 1.27 -2.54)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 3.81)
          (xy -1.27 1.27)
          (xy 1.27 2.54)
          (xy -1.27 3.81)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.032 5.08)
          (xy 3.556 6.604)
          (xy 2.794 6.604)
          (xy 3.556 6.604)
          (xy 3.556 5.842)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.302 4.064)
          (xy 4.826 5.588)
          (xy 4.064 5.588)
          (xy 4.826 5.588)
          (xy 4.826 4.826)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 0 0) (radius 4.572)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "Dual_Blue{slash}Yellow_1_1"
      (pin passive line (at -7.62 2.54 0) (length 3.048)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -2.54 0) (length 3.048)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 2.54 180) (length 3.81)
        (name "K1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -2.54 180) (length 3.81)
        (name "K2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Dual_Red{slash}Green" (extends "Dual_Blue{slash}Yellow")
    (property "Reference" "D" (id 0) (at 0 5.715 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Dual_Red{slash}Green" (id 1) (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "LED_SMD:LED_RGB_Wuerth-PLCC4_3.2x2.8mm_150141M173100" (id 2) (at 0 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0.762 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "LED diode bicolor dual" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Bicolor LED, red and green, 150141RV73100" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
)
